;=======================================================
; P24-8_WS.INF Ver. 1.0 11/17/2017
;
; Monitor INF file for Fujitsu Display P24-8 WS
;
; Copyright 2017 Fujitsu Technology Solutions GmbH
;=======================================================

[Version]
Signature   = "$Windows NT$"
Class       = Monitor
ClassGuid   = {4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider    = %FTS-Mfg%
CatalogFile = P24-8_WS.cat
DriverVer   = 11/17/2017, 1.0.0.0

[SourceDisksNames]
1 = %DiskName%

[SourceDisksFiles]
P24-8.icm = 1

[DestinationDirs]
DefaultDestDir   = 12
P24-8_WS.Copyfiles = 23

[ControlFlags]
ExcludeFromSelect = Monitor\FUS08A2
ExcludeFromSelect = Monitor\FUS08A3
ExcludeFromSelect = Monitor\FUS08A4

[Manufacturer]
%FTS-Mfg% = FTS-Mfg, NTx86, NTAMD64

[FTS-Mfg]
%P24-8_WS.DVI%  = P24-8_WS.DVI.Install, Monitor\FUS08A2
%P24-8_WS.HDMI% = P24-8_WS.HDMI.Install, Monitor\FUS08A3
%P24-8_WS.DP%   = P24-8_WS.DP.Install, Monitor\FUS08A4

[FTS-Mfg.NTx86]
%P24-8_WS.DVI%  = P24-8_WS.DVI.Install, Monitor\FUS08A2
%P24-8_WS.HDMI%  = P24-8_WS.HDMI.Install, Monitor\FUS08A3
%P24-8_WS.DP%     = P24-8_WS.DP.Install, Monitor\FUS08A4

[FTS-Mfg.NTAMD64]
%P24-8_WS.DVI%  = P24-8_WS.DVI.Install, Monitor\FUS08A2
%P24-8_WS.HDMI%  = P24-8_WS.HDMI.Install, Monitor\FUS08A3
%P24-8_WS.DP%     = P24-8_WS.DP.Install, Monitor\FUS08A4

[P24-8_WS.DVI.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P24-8_WS.DVI.AddReg, 1920x1200, DPMS
CopyFiles = P24-8_WS.CopyFiles

[P24-8_WS.HDMI.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P24-8_WS.HDMI.AddReg, 1920x1200, DPMS
CopyFiles = P24-8_WS.CopyFiles

[P24-8_WS.DP.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = P24-8_WS.DP.AddReg, 1920x1200, DPMS
CopyFiles = P24-8_WS.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[P24-8_WS.DVI.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30-82,48-76,+,-"
HKR,,ICMProfile,0,"P24-8.icm"

[P24-8_WS.HDMI.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30-82,50-75,+,-"
HKR,,ICMProfile,0,"P24-8.icm"

[P24-8_WS.DP.AddReg]
HKR,"MODES\1920,1200",Mode1,,"30-82,50-75,+,-"
HKR,,ICMProfile,0,"P24-8.icm"

[1920x1200]
HKR,,MaxResolution,,"1920,1200"

[DPMS]
HKR,,DPMS,,1

[P24-8_WS.CopyFiles]
P24-8.icm

[P24-8_WS.DVI.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[P24-8_WS.HDMI.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[P24-8_WS.DP.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Monitor Class Function Driver Service"
FTS-Mfg         = "Fujitsu Technology Solutions"
DiskName        = "Fujitsu Monitor Installation Disk"

P24-8_WS.DVI = "Fujitsu P24-8 WS (DVI)"
P24-8_WS.HDMI= "Fujitsu P24-8 WS (HDMI)"
P24-8_WS.DP  = "Fujitsu P24-8 WS (DP)"
