;Monitor INF file for Fujitsu Display E24-8_TS_Pro
;Copyright 2016 Fujitsu Technology Solutions

[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%FTS_Mfg%
CatalogFile=E24-8_TS_Pro.cat
DriverVer=09/22/2016,1.0.0.0


[ControlFlags]
ExcludeFromSelect.nt=Monitor\FUS0892
ExcludeFromSelect.nt=Monitor\FUS0893
ExcludeFromSelect.nt=Monitor\FUS0894

[DestinationDirs]
DefaultDestDir=11
E24-8_TS_Pro_a.CopyFiles=23
E24-8_TS_Pro_d.CopyFiles=23
E24-8_TS_Pro_dp.CopyFiles=23

[SourceDisksNames]
1=%DiskName%,,,

[SourceDisksFiles]
E24-8_TS_Pro.icm=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys


[Manufacturer]
%FTS_Mfg%=FTS_Mfg,NTAMD64

[FTS_Mfg] 
%E24-8_TS_Pro_a%=E24-8_TS_Pro_a.Install, Monitor\FUS0892
%E24-8_TS_Pro_d%=E24-8_TS_Pro_d.Install, Monitor\FUS0893
%E24-8_TS_Pro_dp%=E24-8_TS_Pro_dp.Install, Monitor\FUS0894

[FTS_Mfg.NTAMD64] 
%E24-8_TS_Pro_a%=E24-8_TS_Pro_a.Install, Monitor\FUS0892
%E24-8_TS_Pro_d%=E24-8_TS_Pro_d.Install, Monitor\FUS0893
%E24-8_TS_Pro_dp%=E24-8_TS_Pro_dp.Install, Monitor\FUS0894


[E24-8_TS_Pro_a.Install]
DELReg=DEL_CURRENT_REG    
AddReg=E24-8_TS_Pro_a.AddReg
CopyFiles=E24-8_TS_Pro_a.CopyFiles

[E24-8_TS_Pro_a.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[E24-8_TS_Pro_d.Install]
DELReg=DEL_CURRENT_REG    
AddReg=E24-8_TS_Pro_d.AddReg
CopyFiles=E24-8_TS_Pro_d.CopyFiles

[E24-8_TS_Pro_d.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[E24-8_TS_Pro_dp.Install]
DELReg=DEL_CURRENT_REG    
AddReg=E24-8_TS_Pro_dp.AddReg
CopyFiles=E24-8_TS_Pro_dp.CopyFiles

[E24-8_TS_Pro_dp.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install


[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile


[E24-8_TS_Pro_a.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,48.0-76.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"E24-8_TS_Pro.icm"


[E24-8_TS_Pro_d.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,48.0-76.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"E24-8_TS_Pro.icm"

[E24-8_TS_Pro_dp.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,48.0-76.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"E24-8_TS_Pro.icm"


[E24-8_TS_Pro_a.CopyFiles]
E24-8_TS_Pro.icm

[E24-8_TS_Pro_d.CopyFiles]
E24-8_TS_Pro.icm

[E24-8_TS_Pro_dp.CopyFiles]
E24-8_TS_Pro.icm


[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

DiskName="Fujitsu Driver & Utilities CD E24-8 TS Pro"
FTS_Mfg="Fujitsu Technology Solutions"	

E24-8_TS_Pro_a="Fujitsu E24-8 TS Pro (Analog)"
E24-8_TS_Pro_d="Fujitsu E24-8 TS Pro (Digital)"
E24-8_TS_Pro_dp="Fujitsu E24-8 TS Pro (DisplayPort)"