; NETAMD.INF
;
; NDIS5 Driver installation file for AMD PCnet Based Ethernet Adapters.
;
; Copyright 2004-2005, Advanced Micro Devices, Inc.

[version]
CatalogFile = PCNTPCI5.cat
Signature   = "$Windows NT$"
Compatible  = 1 ; added
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %AMD%
;LayoutFile  = layout.inf
DriverVer   = 07/07/2004,4.51.0.0 

[Manufacturer]
;%AMD%    = AMD
%AMD.NT.5.1% = AMD.NT.5.1 ;added
;%Allied% = Allied;, NT.5.1 ; added
%Allied.NT.5.1% = Allied.NT.5.1
;%HP%     = HP;
%HP.NT.5.1% = HP.NT.5.1 ;added
;%IBM%    = IBM 
%IBM.NT.5.1%    = IBM.NT.5.1 

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = "AMD Driver Disk 1",,,

[SourceDisksFiles]
;
; filename_on_source = diskID[, [subdir][, size]]
;
PCNTPCI5.sys = 1,, ; on distribution disk 1


[AMD]

%PCIGENERIC.DeviceDesc% =PCIpcnet.ndi, PCI\VEN_1022&DEV_2000   ;AMD PCnet PCI
;%PCIGENERIC.DeviceDesc% =PCIpcnet.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_20001022    ;AMD PCnet PCI

;added for xp
[AMD.NT.5.1]
%PCIGENERICXP.DeviceDesc% =PCIpcnetxp.ndi, PCI\VEN_1022&DEV_2000   ;AMD PCnet PCI


[Allied]
%*AT2700TX.DeviceDesc%=AT2700TX.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_27001259
%*AT2700FX.DeviceDesc%=AT2700FX.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_27011259
%*AT2450V3.DeviceDesc%=AT2450V3.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_24531259

; added for xp
[Allied.NT.5.1]
%*AT2700TXXP.DeviceDesc%=AT2700TXXP.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_27001259
%*AT2700FXXP.DeviceDesc%=AT2700FXXP.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_27011259
%*AT2450V3XP.DeviceDesc%=AT2450V3XP.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_24531259

[IBM]
%*IBM.DeviceDesc% =  IBM.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_20001014
%*IBM1.DeviceDesc% = IBM1.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_01331014

; added for XP
[IBM.NT.5.1]
%*IBMXP.DeviceDesc% =  IBMXP.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_20001014
%*IBM1XP.DeviceDesc% = IBM1XP.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_01331014


[HP]
%*HPTWEETY.DeviceDesc%  = HPTWEETY.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_104C103C, ; HP Ethernet with LAN remote power adapter
%*HPWOODY.DeviceDesc%   = HPWOODY.ndi,  PCI\VEN_1022&DEV_2000&SUBSYS_1064103C, ; HP Ethernet with LAN remote power adapter
%*HPSQUEEZY.DeviceDesc% = HPSQUEEZY.ndi,PCI\VEN_1022&DEV_2000&SUBSYS_1065103C, ; HP Ethernet with LAN remote power adapter              
%*HPCASPER.DeviceDesc%  = HPCASPER.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_106C103C, ; HP Ethernet with LAN remote power adapter
%*HPPONGO.DeviceDesc%   = HPPONGO.ndi,  PCI\VEN_1022&DEV_2000&SUBSYS_106E103C, ; HP Ethernet with LAN remote power adapter              
%*HPSATAN.DeviceDesc%   = HPSATAN.ndi,  PCI\VEN_1022&DEV_2000&SUBSYS_10EA103C, ; HP Ethernet with LAN remote power adapter              

; added for xp
[HP.NT.5.1]
%*HPTWEETYXP.DeviceDesc%  = HPTWEETYXP.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_104C103C, ; HP Ethernet with LAN remote power adapter
%*HPWOODYXP.DeviceDesc%   = HPWOODYXP.ndi,  PCI\VEN_1022&DEV_2000&SUBSYS_1064103C, ; HP Ethernet with LAN remote power adapter
%*HPSQUEEZYXP.DeviceDesc% = HPSQUEEZYXP.ndi,PCI\VEN_1022&DEV_2000&SUBSYS_1065103C, ; HP Ethernet with LAN remote power adapter              
%*HPCASPERXP.DeviceDesc%  = HPCASPERXP.ndi, PCI\VEN_1022&DEV_2000&SUBSYS_106C103C, ; HP Ethernet with LAN remote power adapter
%*HPPONGOXP.DeviceDesc%   = HPPONGOXP.ndi,  PCI\VEN_1022&DEV_2000&SUBSYS_106E103C, ; HP Ethernet with LAN remote power adapter              
%*HPSATANXP.DeviceDesc%   = HPSATANXP.ndi,  PCI\VEN_1022&DEV_2000&SUBSYS_10EA103C, ; HP Ethernet with LAN remote power adapter              

[CoNTrolFlags]
ExcludeFromSelect=PCI\VEN_1022&DEV_2000, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_20001014, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_104C103C, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_1064103C, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_1065103C, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_106C103C, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_106E103C, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_10EA103C, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_27001259, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_01331014, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_27011259, \
		    PCI\VEN_1022&DEV_2000&SUBSYS_24531259

;****************************************************************************
; ATI AT-2700TX 10/100 PCI Ethernet Adapter
;****************************************************************************
; NT 5.0 section
[AT2700TX.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[AT2700TX.ndi.NTx86.Services]
DelService	= PCnet ; added for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

;added for XP
[AT2700TXXP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[AT2700TXXP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section
[AT2700TXXP.ndi]
AddReg=AT2700TX.ndi.reg,PCnet.Win.reg, DefaultP.reg, DefaultF.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[AT2700TX.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_27001259"
;****************************************************************************
; ATI AT-2700FX 100Mb PCI Ethernet Adapter
;****************************************************************************
[AT2700FX.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[AT2700FX.ndi.NTx86.Services]
DelService	= PCnet ; added for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; added for xp
[AT2700FXXP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[AT2700FXXP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section
[AT2700FXXP.ndi]
AddReg=AT2700FX.ndi.reg,PCnet.Win.reg, DefaultP.reg, DefaultF.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[AT2700FX.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_27011259"

;****************************************************************************
; ATI AT-2450v3 PCI Ethernet Adapter
;****************************************************************************
[AT2450V3.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[AT2450V3.ndi.NTx86.Services]
DelService	= PCnet ; added for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

;added for XP
[AT2450V3XP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[AT2450V3XP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section
[AT2450V3XP.ndi]
AddReg=AT2450V3.ndi.reg,PCnet.Win.reg, DefaultP.reg, DefaultF.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[AT2450V3.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_24531259"
;****************************************************************************
; IBMPCI   ;IBM
;****************************************************************************
; NT 5.0 section
[IBM.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[IBM.ndi.NTx86.Services]
DelService	= PCnet ;added for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

;added for xp
[IBMXP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[IBMXP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section
[IBMXP.ndi]
AddReg = IBM.ndi.reg,PCnet.Win.reg, DefaultP.reg, DefaultF.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[IBM.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_20001014"
;****************************************************************************
; IBMPCI   ;IBM iSeries 10/100 adapter
;****************************************************************************
; NT 5.0 section
[IBM1.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[IBM1.ndi.NTx86.Services]
DelService      = PCnet ; added for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

;added for XP
[IBM1XP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[IBM1XP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section
[IBM1XP.ndi]
AddReg = IBM1.ndi.reg,PCnet.Win.reg, DefaultP.reg, DefaultF.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[IBM1.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_01331014"
;****************************************************************************
; HP Pcnet PCI      ;AMD pcNET PCI
;****************************************************************************
; NT5.0 section for Tweety
[HPTWEETY.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPTWEETY.ndi.NTx86.Services]
DelService	= PCnet ; aded for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; added for XP
[HPTWEETYXP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPTWEETYXP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section for Tweety
[HPTWEETYXP.ndi]
AddReg = HPTWEETY.ndi.reg,PCnet.Win.reg, HPDefaultP.reg, DefaultF.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[HPTWEETY.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_104C103C"

; NT5.0 section for Woody
[HPWOODY.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPWOODY.ndi.NTx86.Services]
DelService	= PCnet ; aded for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

;added for XP
[HPWOODYXP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPWOODYXP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section for Woody
[HPWOODYXP.ndi]
AddReg = HPWOODY.ndi.reg,PCnet.Win.reg, HPDefaultP.reg, DefaultF.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[HPWOODY.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_1064103C"

; NT5.0 section for Squeezy
[HPSQUEEZY.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPSQUEEZY.ndi.NTx86.Services]
DelService	= PCnet ; added for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

;added for xp
[HPSQUEEZYXP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPSQUEEZYXP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section for Squeezy
[HPSQUEEZYXP.ndi]
AddReg = HPSQUEEZY.ndi.reg,PCnet.Win.reg, HPDefaultP.reg, DefaultF.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[HPSQUEEZY.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_1065103C"

; NT5.0 section for Casper
[HPCASPER.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPCASPER.ndi.NTx86.Services]
DelService	= PCnet ;added for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

;added for xp
[HPCASPERXP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPCASPERXP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section for Casper
[HPCASPERXP.ndi]
AddReg = HPCASPER.ndi.reg,PCnet.Win.reg, HPDefaultP.reg, DefaultF.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[HPCASPER.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_106C103C"

; NT5.0 section for Pongo
[HPPONGO.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPPONGO.ndi.NTx86.Services]
DelService	= PCnet ; added for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; added for xp
[HPPONGOXP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPPONGOXP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section for Pongo
[HPPONGOXP.ndi]
AddReg = HPPONGO.ndi.reg,PCnet.Win.reg, HPDefaultP.reg, DefaultF.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[HPPONGO.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_106E103C"

; NT5.0 section for SATANAS
[HPSATAN.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPSATAN.ndi.NTx86.Services]
DelService	= PCnet ; added for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

;added for xp
[HPSATANXP.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, HPDefaultP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[HPSATANXP.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x section for SATAN
[HPSATANXP.ndi]
AddReg = HPSATAN.ndi.reg,PCnet.Win.reg, HPDefaultP.reg, DefaultF.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles

[HPSATAN.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000&SUBSYS_106E103C"
;****************************************************************************
; PCIpcnet       ;AMD pcNET PCI
;****************************************************************************
; NT5.0 Section
[PCIpcnet.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[PCIpcnet.ndi.NTx86.Services]
DelService	= PCnet ; added  for IBM
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

;added for xp
[PCIpcnetxp.ndi.NTx86]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = PCnet.NT.reg, DefaultP.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.CopyFiles

[PCIpcnetxp.ndi.NTx86.Services]
AddService      = PCnet, 2, PCnet.Service, PCnet.AddEveNTLog

; Win9x Section
[PCIpcnetxp.ndi]
AddReg = PCIpcnet.ndi.reg,PCnet.Win.reg, DefaultP.reg, DefaultF.reg, BasicP.reg, MIIP.reg
CopyFiles       = PCnet.ndis3.CopyFiles 

[PCIpcnet.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1022&DEV_2000"

;-------------------------------------------------------------------------------
; Common Section for NT5.0 and Win9x.
;-------------------------------------------------------------------------------
;
; AMD common params section
;
[DefaultP.reg]
HKR, ,                              BUS_TO_SCAN,        0, "ALL"
HKR, ,                              BUSTIMER,           0, "0"
HKR, ,                              LED0,                       0, "10000"
HKR, ,                              LED1,                       0, "10000"
HKR, ,                              LED2,                       0, "10000"
HKR, ,                              LED3,                       0, "10000"
HKR, ,                              TP,                         0, "0"
HKR, ,                              FDUP,                     0, "0"
HKR, ,                              MPMODE,                     0, "0"
HKR, ,                              Priority8021p,      0, "0"
HKR, ,                              TcpipOffload,      0, "0"
HKR, ,                              EXTPHY,                     0, "0"

[BasicP.reg]
HKR, Ndi\params\TP,                 ParamDesc,   0, %TP%
HKR, Ndi\params\TP,                 default,     0, "0"
HKR, Ndi\params\TP,                 type,        0, "enum"
HKR, Ndi\params\TP\enum,            "0",         0, %OFF%
HKR, Ndi\params\TP\enum,            "1",         0, %(Default)ON%

HKR, Ndi\params\FDUP,               ParamDesc,   0, %FDUP% 
HKR, Ndi\params\FDUP,               default,     0, "0"
HKR, Ndi\params\FDUP,               type,        0, "enum"
HKR, Ndi\params\FDUP\enum,          "0",         0, %Default%
HKR, Ndi\params\FDUP\enum,          "1",         0, %OFF%
HKR, Ndi\params\FDUP\enum,          "2",         0, %AUIFD%
HKR, Ndi\params\FDUP\enum,          "3",         0, %UTPFD%
HKR, Ndi\params\FDUP\enum,          "4",         0, %FIBER%


HKR, Ndi\params\MPMODE,             ParamDesc,   0, %MPMODE%
HKR, Ndi\params\MPMODE,             default,     0, "0"
HKR, Ndi\params\MPMODE,             type,        0, "enum"
HKR, Ndi\params\MPMODE\enum,        "0",         0, %Default(OFF)%
HKR, Ndi\params\MPMODE\enum,        "1",         0, %ON%

HKR, Ndi\params\Priority8021p,             ParamDesc,   0, %Priority8021p%
HKR, Ndi\params\Priority8021p,             default,     0, "0"
HKR, Ndi\params\Priority8021p,             type,        0, "enum"
HKR, Ndi\params\Priority8021p\enum,        "0",         0, %Default(OFF)%
HKR, Ndi\params\Priority8021p\enum,        "1",         0, %ON%

; Network Address
HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"

HKR, Ndi\params\TcpipOffload,             ParamDesc,   0, %TcpipOffload%
HKR, Ndi\params\TcpipOffload,             default,     0, "0"
HKR, Ndi\params\TcpipOffload,             type,        0, "enum"
HKR, Ndi\params\TcpipOffload\enum,        "0",         0, %Default(OFF)%
HKR, Ndi\params\TcpipOffload\enum,        "1",         0, %ON%

[MIIP.reg]
HKR, Ndi\params\EXTPHY,             ParamDesc,   0, %EXTPHY%
HKR, Ndi\params\EXTPHY,             default,     0, "0"
HKR, Ndi\params\EXTPHY,             type,        0, "enum"
HKR, Ndi\params\EXTPHY\enum,        "0",         0, %Auto%
HKR, Ndi\params\EXTPHY\enum,        "1",         0, %100HD%
HKR, Ndi\params\EXTPHY\enum,        "2",         0, %100FD%
HKR, Ndi\params\EXTPHY\enum,        "3",         0, %10HD%
HKR, Ndi\params\EXTPHY\enum,        "4",         0, %10FD%

;
; HP only params section
;
[HPDefaultP.reg]
HKR, ,                              BUS_TO_SCAN, 0, "ALL"
HKR, ,                              BUSTIMER,    0, "0"
HKR, ,                              LED0,        0, "10000"
HKR, ,                              LED1,        0, "10000"
HKR, ,                              LED2,        0, "90"
HKR, ,                              LED3,        0, "10000"
HKR, ,                              TP,          0, "1"
HKR, ,                              MPMODE,      0, "0"
HKR, ,                              Priority8021p,      0, "0"
HKR, ,                              TcpipOffload,      0, "0"
HKR, ,                              EXTPHY,      0, "0"

[PCnet.CopyFiles]
PCNTPCI5.sys,,,2

;-------------------------------------------------------------------------------
; NT 5.0 only sections
;-------------------------------------------------------------------------------

[PCnet.NT.reg]
HKR, Ndi,            Service,    0, "PCnet"
;HKR, Ndi\INTerfaces, DefUpper,   0, "ndis5"
;HKR, Ndi\INTerfaces, DefLower,   0, "ethernet"
HKR, Ndi\INTerfaces, UpperRange, 0, "ndis5"
HKR, Ndi\INTerfaces, LowerRange, 0, "ethernet"

[PCnet.Service]
DisplayName     = %PCnet.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorCoNTrol    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\PCNTPCI5.sys
LoadOrderGroup  = NDIS
AddReg          = TextModeFlags.reg

[PCnet.AddEveNTLog]
AddReg = PCnet.AddEveNTLog.reg

[PCnet.AddEveNTLog.reg]
HKR, , EveNTMessageFile, 0x00020000, "%%SystemRoot%%\System32\neteveNT.dll"
HKR, , TypesSupported,   0x00010001, 7


[TextModeFlags.reg]
HKR,  , TextModeFlags, 0x00010001, 0x0001

;-------------------------------------------------------------------------------
; Win9x only sections
;-------------------------------------------------------------------------------
[DefaultF.reg]
;HKR,NDI\params\BUS_TO_SCAN,flag,1,30,00,00,00
;HKR,NDI\params\BUSTIMER,flag,1,30,00,00,00
HKR,NDI\params\FDUP,flag,1,20,00,00,00
;HKR,NDI\params\LED0,flag,1,30,00,00,00
;HKR,NDI\params\LED1,flag,1,30,00,00,00
;HKR,NDI\params\LED2,flag,1,30,00,00,00
;HKR,NDI\params\LED3,flag,1,30,00,00,00
HKR,NDI\params\MPMODE,flag,1,20,00,00,00
HKR,NDI\params\Priority8021p,flag,1,20,00,00,00
HKR,NDI\params\TcpipOffload,flag,1,20,00,00,00
HKR,NDI\params\TP,flag,1,20,00,00,00
HKR,NDI\params\EXTPHY,flag,1,20,00,00,00

[PCnet.Win.reg]
; key,subkey,valuname,type,value
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,PCNTPCI5.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"

; NDIS Info
HKR,NDIS,LogDriverName,,"PCnet"
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0a

; INTerfaces
HKR,Ndi\INTerfaces,DefUpper,,"ndis3"
HKR,Ndi\INTerfaces,DefLower,,"ethernet"
HKR,Ndi\INTerfaces,UpperRange,,"ndis3"
HKR,Ndi\INTerfaces,LowerRange,,"ethernet"

; Install
HKR,Ndi\Install,ndis3,,"PCnet.ndis3"

[PCnet.ndis3.CopyFiles]
PCNTPCI5.sys,,,2

;-------------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
PCnet.CopyFiles = 12
PCnet.ndis3.CopyFiles = 11
;PCnet.inf.CopyFiles = 17

;-------------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
;Msft			 + "Microsoft"
AMD                      = "AMD Inc."
Allied                   = "Allied Telesyn"
HP                       = "HP"
IBM                      = "IBM"
AMD.NT.5.1		 = "AMD Inc."
Allied.NT.5.1            = "Allied"
HP.NT.5.1 		 = "HP" ;added
IBM.NT.5.1    		 = "IBM"
TP                       = "TP Mode"
Default                  = "Use Adapter Setting"
OFF                      = "Off"
(Default)ON              = "On (Default)"
Default(OFF)             = "Off (Default)"
ON                       = "On"
MPMODE                   = "MP Mode"
Priority8021p            = "IEEE 802.1p Tagging"
NetworkAddress           = "Locally Administered Address"
TcpipOffload             = "TCP/IP Offload"
FDUP                     = "Full Duplex"
EXTPHY                   = "External PHY"
Auto                     = "Auto Detect"
AUIFD                    = "AUI - Full Duplex"
UTPFD                    = "UTP - Full Duplex"
FIBER                    = "Fiber NIC"
100HD                    = "100Mbps Half Duplex"
100FD                    = "100Mbps Full Duplex"
10HD                     = "10Mbps Half Duplex"
10FD                     = "10Mbps Full Duplex"

PCIGENERIC.DeviceDesc    = "AMD PCNET Family Ethernet Adapter (PCI)"

;added for XP
PCIGENERICXP.DeviceDesc    = "AMD PCNET Family Ethernet Adapter (PCI)"


*AT2700TX.DeviceDesc     = "Allied Telesyn AT-2700TX PCI 10/100 Ethernet Adapter"
*AT2700FX.DeviceDesc     = "Allied Telesyn AT-2700FX PCI 100Mb Ethernet Adapter"
*AT2450V3.DeviceDesc     = "Allied Telesyn AT-2450v3 PCI Ethernet Adapter"

;added for xp
*AT2700TXXP.DeviceDesc     = "Allied Telesyn AT-2700TX PCI 10/100 Ethernet Adapter"
*AT2700FXXP.DeviceDesc     = "Allied Telesyn AT-2700FX PCI 100Mb Ethernet Adapter"
*AT2450V3XP.DeviceDesc     = "Allied Telesyn AT-2450v3 PCI Ethernet Adapter"

*IBM.DeviceDesc          = "IBM 10/100 NetFinity Fault ToleraNT Adapter"
*IBM1.DeviceDesc         = "IBM iSeries 10/100 adapter"

;added for XP
*IBMXP.DeviceDesc          = "IBM 10/100 NetFinity Fault ToleraNT Adapter"
*IBM1XP.DeviceDesc         = "IBM iSeries 10/100 adapter"

*HPTWEETY.DeviceDesc     = "HP Ethernet with LAN remote power adapter"
*HPWOODY.DeviceDesc      = "HP Ethernet with LAN remote power adapter"
*HPSQUEEZY.DeviceDesc    = "HP Ethernet with LAN remote power adapter"
*HPCASPER.DeviceDesc     = "HP Ethernet with LAN remote power adapter"
*HPPONGO.DeviceDesc      = "HP Ethernet with LAN remote power adapter"
*HPSATAN.DeviceDesc      = "HP Ethernet with LAN remote power adapter"

;added for xp
*HPTWEETYXP.DeviceDesc     = "HP Ethernet with LAN remote power adapter"
*HPWOODYXP.DeviceDesc      = "HP Ethernet with LAN remote power adapter"
*HPSQUEEZYXP.DeviceDesc    = "HP Ethernet with LAN remote power adapter"
*HPCASPERXP.DeviceDesc     = "HP Ethernet with LAN remote power adapter"
*HPPONGOXP.DeviceDesc      = "HP Ethernet with LAN remote power adapter"
*HPSATANXP.DeviceDesc      = "HP Ethernet with LAN remote power adapter"

PCnet.Service.DispName   = "PCNET Adapter Driver"
