;******************************************************************************
; NETCBE.INF
;
; Xircom CardBus Ethernet 10/100 Network Adapters
; Installation File for Windows 95, 98 and 2000
; Supports NDIS3, NDIS4 and NDIS5 drivers
;
; Copyright (c) 1998 - 2000 Xircom, Inc. All Rights Reserved
;
; $Date:   21 Nov 2001 11:15:22  $
; $Revision:   1.36  $
;
;------------------------------------------------------------------------------

;******************************************************************************
; Version Section
;------------------------------------------------------------------------------
[Version]
Signature	= "$Chicago$"
Compatible	= 1
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer	= 11/21/2001, 3.14.11.0
Provider	= %COMPANY_NAME%
CatalogFile	= NETCBE.CAT

;******************************************************************************
; Manufacturer
;------------------------------------------------------------------------------
[Manufacturer]
%COMPANY_NAME% = Device

[ControlFlags]
ExcludeFromSelect = PCI\VEN_1011&DEV_0019&SUBSYS_0002115D, \
                    PCI\VEN_115D&DEV_0003&SUBSYS_0181115D, \
                    PCI\VEN_115D&DEV_0003&SUBSYS_1181115D, \
                    PCI\VEN_115D&DEV_0003&SUBSYS_0182115D, \
		    PCI\VEN_115D&DEV_0003&SUBSYS_1182115D

;******************************************************************************
; Device
;------------------------------------------------------------------------------
[Device]
%NIC1%		= Install_NIC1,PCI\VEN_1011&DEV_0019&SUBSYS_0002115D    ; CBE
%NIC2%		= Install_NIC2,PCI\VEN_115D&DEV_0003&SUBSYS_0181115D    ; CBE2
%NIC3%		= Install_NIC2,PCI\VEN_115D&DEV_0003&SUBSYS_1181115D    ; CBEM
%NIC4%		= Install_NIC2,PCI\VEN_115D&DEV_0003&SUBSYS_0182115D    ; R2BE
%NIC5%		= Install_NIC2,PCI\VEN_115D&DEV_0003&SUBSYS_1182115D    ; R2BEM
%NIC_ML%	= Install_NIC_ML, %NIC_ML_ID% ; Non PnP DeviceID, necessary for retail WIN95

;******************************************************************************
; Install
;------------------------------------------------------------------------------

[Install_NIC1]          ; CBE
AddReg    = Addreg_NDIS, Addreg_NIC, Addreg_NIC1, Addreg_NIC_Params
DelReg    = Delreg_NIC1_Params
CopyFiles = CopyFiles_NIC 

[Install_NIC1.NT]
AddReg          = Addreg_NIC_Params, nt_reg
DelReg          = Delreg_NICNT_Params
Characteristics = 0x84   ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5      ; PCI
CopyFiles       = NIC_CopyFiles

[Install_NIC1.NT.Services]
AddService = CBEN5, 2, NIC_Service, common_EventLog

[Install_NIC2]          ; CBE2/CBEM/R2BE/R2BEM
AddReg    = Addreg_NDIS, Addreg_NIC, Addreg_NIC2, Addreg_NIC_Params
DelReg    = Delreg_NIC1_Params
CopyFiles = CopyFiles_NIC

[Install_NIC2.NT]
AddReg          = Addreg_NIC_Params, nt_reg
DelReg          = Delreg_NICNT_Params
Characteristics = 0x84   ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5      ; PCI
CopyFiles       = NIC_CopyFiles

[Install_NIC2.NT.Services]
AddService = CBEN5, 2, NIC_Service, common_EventLog

[Install_NIC_ML]        ; WIN95 forced load support
AddReg    = Addreg_NDIS, Addreg_NIC, Addreg_NIC_ML, Addreg_NIC_Params, Addreg_NIC_ML_Params
LogConfig = LogConfig_IO, LogConfig_MEM

; NT section to keep CHKINF from checking our Install_NIC_ML section
[Install_NIC_ML.NT]
AddReg    = nt_reg
DelReg          = Delreg_NICNT_Params
Characteristics = 0x84   ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType         = 1      ; ISA

; NT section to keep CHKINF from checking our Install_NIC_ML section
[Install_NIC_ML.NT.Services]
AddService = CBEN5, 2, NIC_Service

;******************************************************************************
; Add Registry
;------------------------------------------------------------------------------
[Addreg_NDIS]				               ; W9x Only Registry Entries
HKR,    ,DevLoader,     ,"*ndis"
HKR,    ,DeviceVxDs,    ,%NIC_DRIVERNAME%
HKR,    ,EnumPropPages, ,"netdi.dll,EnumPropPages"
HKR,	,Mode,		,"IO"

; NDIS Info
HKR,NDIS,LogDriverName,,%NIC_LOGDRIVERNAME%
HKR,NDIS,MajorNdisVersion,1,5
HKR,NDIS,MinorNdisVersion,1,0

; Interfaces
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"

; Install
HKR,Ndi\Install,ndis5,,"Copyfiles"
HKR,Ndi,NdiInstaller,,"NDIW9X.DLL,NdiW9xProc"

; Help section
HKR,Ndi,HelpText,,%NIC_HELP%

; NDIS Switcher
HKR,                      ,     AUTO       , ,"NOTSET"
HKR,                      ,     NDIS5      , ,"CBEN5.SYS"
HKR,                      ,     NDIS4      , ,"CBEN4.SYS"
HKR,                      ,     NDIS3      , ,"CBE.SYS"
HKR,                      ,     KeyWords   , ,"PacketPriority"
HKR,                      ,     NdisVersion, ,"AUTO"

; NDIS Version Keyword
HKR,Ndi\params\NdisVersion,     ParamDesc  ,0, "NdisVersion"
HKR,Ndi\params\NdisVersion,     type       ,0, "enum"
HKR,Ndi\params\NdisVersion,     default    ,0, "AUTO"
HKR,Ndi\params\NdisVersion\enum,"AUTO"     ,0, "Auto Select"
HKR,Ndi\params\NdisVersion\enum,"NDIS3"    ,0, "NDIS 3"
HKR,Ndi\params\NdisVersion\enum,"NDIS4"    ,0, "NDIS 4"
HKR,Ndi\params\NdisVersion\enum,"NDIS5"    ,0, "NDIS 5"

; PacketPriority Entries for NDIS Switcher
HKR, Ndi\Params\PacketPriority, "NDIS3"    ,0, "0"
HKR, Ndi\Params\PacketPriority, "NDIS4"    ,0, "0"
HKR, Ndi\Params\PacketPriority, "NDIS5"    ,0, "0,1"
HKR, Ndi\Params\PacketPriority, "NSOS"     ,0, "95,95R2,98"

[Addreg_NIC]
HKR,,InterruptNumber,1,04,00,00,00
HKR,,IoBaseAddress,1,02,00,00,00
HKR,,MemoryBaseAddress,1,01,00,00,00

[Addreg_NIC1]
HKR,Ndi,DeviceID,,"PCI\VEN_1011&DEV_0019"       

[Addreg_NIC2]
HKR,Ndi,DeviceID,,"PCI\VEN_115D&DEV_0003"

[Addreg_NIC_ML]					; WIN95 forced load support
HKR,Ndi,CardType,,"LEGACY"
HKR,Ndi,DeviceID,,%NIC_ML_ID%			; Non PNP DeviceID, necessary for SR1 WIN95
   		
;******************************************************************************
; Logical Configurations
;------------------------------------------------------------------------------
[LogConfig_MEM]
ConfigPriority=NORMAL
IRQConfig=S:3,4,5,6,7,8,9,10,11,12,13,14,15
MemConfig=1000@C0000-FFFFF%FFFFC000, 1000@10000000-FFFFFFFF%FFFFC000
MemConfig=1000@C0000-FFFFF%FFFFC000, 1000@10000000-FFFFFFFF%FFFFC000

[LogConfig_IO]
ConfigPriority=DESIRED
IRQConfig=S:3,4,5,6,7,8,9,10,11,12,13,14,15
MemConfig=1000@C0000-FFFFF%FFFFC000, 1000@10000000-FFFFFFFF%FFFFC000
MemConfig=1000@C0000-FFFFF%FFFFC000, 1000@10000000-FFFFFFFF%FFFFC000
IOConfig=80@100-FFFFFF7F%FFFFFF80

;******************************************************************************
; Windows 2000 specific info
;------------------------------------------------------------------------------

[nt_reg]
HKR, Ndi\Interfaces,     UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,     LowerRange, 0, "ethernet"
HKR, Ndi,                Service,    0, "CBEN5"

[NIC_Service]
DisplayName     = %NIC_Service_DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\cben5.sys
LoadOrderGroup  = NDIS

[common_EventLog]
AddReg = common_AddEventLog_reg

[common_AddEventLog_reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\cben5.sys"
HKR, , TypesSupported,   0x00010001, 7

;******************************************************************************
; Copy file sections
;------------------------------------------------------------------------------

[NIC_CopyFiles]
cben5.sys,,,2

[CopyFiles_NIC]
;ndiw9x.dll
;cbe.sys
;cben4.sys
cben5.sys

;******************************************************************************
; Source Disk Names & Source Disk Files
;------------------------------------------------------------------------------
[SourceDisksNames]
1=%NETWORK_DISK%,,, .\

[SourceDisksFiles]
%NIC_DRIVERNAME% = 1
CBE.SYS      = 1
CBEN4.SYS    = 1
CBEN5.SYS    = 1
ndiw9x.dll   = 1

;******************************************************************************
; Destination Directories
;------------------------------------------------------------------------------
[DestinationDirs]
DefaultDestDir	= 11 ; SYSTEM directory
CopyFiles_NIC	= 11 ; SYSTEM directory
NIC_CopyFiles	= 12 ; SYSTEM32\DRIVERS directory

;******************************************************************************
; Localizable Strings
;------------------------------------------------------------------------------
[Strings]
COMPANY_NAME	= "Xircom"
NIC1		= "Xircom CardBus Ethernet 10/100"
NIC2		= "Xircom CardBus Ethernet II 10/100"
NIC3		= "Xircom CardBus Ethernet 100 + Modem 56 (Ethernet Interface)"
NIC4		= "Xircom RealPort2 CardBus Ethernet 10/100"
NIC5		= "Xircom RealPort2 CardBus Ethernet 10/100+Modem 56 (Ethernet Interface)"
NIC_ML		= "Xircom CardBus Ethernet 10/100 Adapter manual load"
NIC_HELP	= "Xircom's CardBus Adapter works in a PCMCIA slot that supports CardBus for full 32-bit support that provides PCI speed in a mobile adapter."
NIC_DRIVERNAME	= "cben5.sys"
NIC_ML_ID	= "XIRCOM-CBE_10/100"

NIC_LOGDRIVERNAME = "CBEN5"
NIC_Service_DispName = "Xircom CardBus Ethernet 10/100 Adapter family"
;--------------------------------------
; Driver Disk names
;--------------------------------------
NETWORK_DISK = "Windows 95, 98 and NT Drivers Disk"

;--------------------------------------
; Context help
;--------------------------------------

;--------------------------------------
; Parameters
;--------------------------------------

NetworkAddress          = "Network Address"
LineConfig              = "Line Configuration"
Negotiation             = "Line Negotiation"
AutoD                   = "Auto Detect"
10HD                    = "10 Mbps/Half Duplex"
10FD                    = "10 Mbps/Full Duplex"
100HD                   = "100 Mbps/Half Duplex"
100FD                   = "100 Mbps/Full Duplex"
ON                      = "On"
OFF                     = "Off"
InitDelay               = "Initialization Delay"
LinkIntegrity           = "Link Integrity"
TxBufferSize            = "Transmit Buffer Size"
RxBufferSize            = "Receive Buffer Size"
CableDetect             = "Cable Detect"
AutoPolarity            = "Auto Polarity"
DynamicLinkDetect       = "Dynamic Link Detect"
PacketPriority          = "Packet Priority"
InterruptStyle          = "InterruptStyle"
PCIIRQ                  = "PCI IRQ"
ISAIRQ                  = "ISA IRQ"
SocketNumber            = "SocketNumber"
Cache                   = "Cache"
Latency                 = "Latency"
DisableBurstMode        = "DisableBurstMode"
DisablePrefetching      = "DisablePrefetching"
DisableWritePosting     = "DisableWritePosting"

;--------------------------------------
; PNP Devices
;--------------------------------------

;******************************************************************************
; Params
;------------------------------------------------------------------------------
[Addreg_NIC_Params]

HKR, Ndi\Params\AutoPolarity,          ParamDesc,  0, %AutoPolarity%
HKR, Ndi\Params\AutoPolarity,          type,       0, "enum"
HKR, Ndi\Params\AutoPolarity,          default,    0, "1"
HKR, Ndi\Params\AutoPolarity\enum,     "1",        0, %ON%
HKR, Ndi\Params\AutoPolarity\enum,     "0",        0, %OFF%

HKR, Ndi\Params\CableDetect,           ParamDesc,  0, %CableDetect%
HKR, Ndi\Params\CableDetect,           type,       0, "enum"
HKR, Ndi\Params\CableDetect,           default,    0, "1"
HKR, Ndi\Params\CableDetect\enum,      "1",        0, %ON%
HKR, Ndi\Params\CableDetect\enum,      "0",        0, %OFF%

HKR, Ndi\Params\DynamicLinkDetect,     ParamDesc,  0, %DynamicLinkDetect%
HKR, Ndi\Params\DynamicLinkDetect,     type,       0, "enum"
HKR, Ndi\Params\DynamicLinkDetect,     default,    0, "1"
HKR, Ndi\Params\DynamicLinkDetect\enum,"1",        0, %ON%
HKR, Ndi\Params\DynamicLinkDetect\enum,"0",        0, %OFF%

HKR, Ndi\Params\InitDelay,             ParamDesc,  0, %InitDelay%
HKR, Ndi\Params\InitDelay,             type,       0, "INT"
HKR, Ndi\Params\InitDelay,             default,    0, "0"
HKR, Ndi\Params\InitDelay,             optional,   0, "1"
HKR, Ndi\Params\InitDelay,             min,        0, "0"
HKR, Ndi\Params\InitDelay,             max,        0, "60"
HKR, Ndi\Params\InitDelay,             step,       0, "1"

HKR, Ndi\Params\LineConfig,            ParamDesc,  0, %LineConfig%
HKR, Ndi\Params\LineConfig,            type,       0, "enum"
HKR, Ndi\Params\LineConfig,            default,    0, "0"
HKR, Ndi\Params\LineConfig\enum,       "0",        0, %AutoD%
HKR, Ndi\Params\LineConfig\enum,       "1",        0, %10HD%
HKR, Ndi\Params\LineConfig\enum,       "2",        0, %10FD%
HKR, Ndi\Params\LineConfig\enum,       "3",        0, %100HD%
HKR, Ndi\Params\LineConfig\enum,       "4",        0, %100FD%

HKR, Ndi\Params\Negotiation,           ParamDesc,  0, %Negotiation%
HKR, Ndi\Params\Negotiation,           type,       0, "enum"
HKR, Ndi\Params\Negotiation,           default,    0, "1"
HKR, Ndi\Params\Negotiation\enum,      "1",        0, %ON%
HKR, Ndi\Params\Negotiation\enum,      "0",        0, %OFF%

HKR, Ndi\Params\LinkIntegrity,         ParamDesc,  0, %LinkIntegrity%
HKR, Ndi\Params\LinkIntegrity,         type,       0, "enum"
HKR, Ndi\Params\LinkIntegrity,         default,    0, "1"
HKR, Ndi\Params\LinkIntegrity\enum,    "1",        0, %ON%
HKR, Ndi\Params\LinkIntegrity\enum,    "0",        0, %OFF%

HKR, Ndi\Params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\Params\NetworkAddress,        type,       0, "edit"
HKR, Ndi\Params\NetworkAddress,        default,    0, ""
HKR, Ndi\Params\NetworkAddress,        LimitText,  0, "12"
HKR, Ndi\Params\NetworkAddress,        UpperCase,  0, "1"
HKR, Ndi\Params\NetworkAddress,        optional,   0, "1"

HKR, Ndi\Params\PacketPriority,        ParamDesc,  0, %PacketPriority%
HKR, Ndi\Params\PacketPriority,        type,       0, "enum"
HKR, Ndi\Params\PacketPriority,        default,    0, "0"
HKR, Ndi\Params\PacketPriority\enum,   "1",        0, %ON%
HKR, Ndi\Params\PacketPriority\enum,   "0",        0, %OFF%

HKR, Ndi\Params\RXBUFFERSIZE,          ParamDesc,  0, %RxBufferSize%
HKR, Ndi\Params\RXBUFFERSIZE,          type,       0, "INT"
HKR, Ndi\Params\RXBUFFERSIZE,          default,    0, "30"
HKR, Ndi\Params\RXBUFFERSIZE,          optional,   0, "1"
HKR, Ndi\Params\RXBUFFERSIZE,          min,        0, "1"
HKR, Ndi\Params\RXBUFFERSIZE,          max,        0, "100"
HKR, Ndi\Params\RXBUFFERSIZE,          step,       0, "1"

HKR, Ndi\Params\TXBUFFERSIZE,          ParamDesc,  0, %TxBufferSize%
HKR, Ndi\Params\TXBUFFERSIZE,          type,       0, "INT"
HKR, Ndi\Params\TXBUFFERSIZE,          default,    0, "10"
HKR, Ndi\Params\TXBUFFERSIZE,          optional,   0, "1"
HKR, Ndi\Params\TXBUFFERSIZE,          min,        0, "1"
HKR, Ndi\Params\TXBUFFERSIZE,          max,        0, "100"
HKR, Ndi\Params\TXBUFFERSIZE,          step,       0, "1"

[Addreg_NIC_ML_Params]
HKR, Ndi\Params\InterruptStyle,        ParamDesc,  0, %InterruptStyle%
HKR, Ndi\Params\InterruptStyle,        type,       0, "enum"
HKR, Ndi\Params\InterruptStyle,        default,    0, "0"
HKR, Ndi\Params\InterruptStyle\enum,   0,          0, %AutoD%
HKR, Ndi\Params\InterruptStyle\enum,   1,          0, %PCIIRQ%
HKR, Ndi\Params\InterruptStyle\enum,   2,          0, %ISAIRQ%

HKR, Ndi\Params\SocketNumber,          ParamDesc,  0, %SocketNumber%
HKR, Ndi\Params\SocketNumber,          default,    0, "0"
HKR, Ndi\Params\SocketNumber,          type,       0, "enum"
HKR, Ndi\Params\SocketNumber\enum,     0,          0, %AutoD%
HKR, Ndi\Params\SocketNumber\enum,     1,          0, "1"
HKR, Ndi\Params\SocketNumber\enum,     2,          0, "2"
HKR, Ndi\Params\SocketNumber\enum,     3,          0, "3"
HKR, Ndi\Params\SocketNumber\enum,     4,          0, "4"

HKR, Ndi\Params\CACHE,                 ParamDesc,  0, %Cache%
HKR, Ndi\Params\CACHE,                 type,       0, "enum"
HKR, Ndi\Params\CACHE,                 default,    0, "32"
HKR, Ndi\Params\CACHE,                 optional,   0, "1"
HKR, Ndi\Params\CACHE\enum,            0,          0, "0"
HKR, Ndi\Params\CACHE\enum,            8,          0, "8"
HKR, Ndi\Params\CACHE\enum,            16,         0, "16"
HKR, Ndi\Params\CACHE\enum,            32,         0, "32"

HKR, Ndi\Params\LATENCY,               ParamDesc,  0, %Latency%
HKR, Ndi\Params\LATENCY,               type,       0, "INT"
HKR, Ndi\Params\LATENCY,               default,    0, "32"
HKR, Ndi\Params\LATENCY,               optional,   0, "1"
HKR, Ndi\Params\LATENCY,               Min,        0, "0"
HKR, Ndi\Params\LATENCY,               Max,        0, "255"
HKR, Ndi\Params\LATENCY,               Step,       0, "1"

HKR, Ndi\Params\NOBURST,               ParamDesc,  0, %DisableBurstMode%
HKR, Ndi\Params\NOBURST,               type,       0, "enum"
HKR, Ndi\Params\NOBURST,               default,    0, "ON"
HKR, Ndi\Params\NOBURST,               optional,   0, "1"
HKR, Ndi\Params\NOBURST\enum,          ON,         0, "ON"

HKR, Ndi\Params\NOPREFETCH,            ParamDesc,  0, %DisablePrefetching%
HKR, Ndi\Params\NOPREFETCH,            type,       0, "enum"
HKR, Ndi\Params\NOPREFETCH,            default,    0, "ON"
HKR, Ndi\Params\NOPREFETCH,            optional,   0, "1"
HKR, Ndi\Params\NOPREFETCH\Enum,       ON,         0, "ON"

HKR, Ndi\Params\NOWRITEPOST,           ParamDesc,  0, %DisableWritePosting%
HKR, Ndi\Params\NOWRITEPOST,           type,       0, "enum"
HKR, Ndi\Params\NOWRITEPOST,           default,    0, "ON"
HKR, Ndi\Params\NOWRITEPOST,           optional,   0, "1"
HKR, Ndi\Params\NOWRITEPOST\Enum,      ON,         0, "ON"

[Delreg_NIC1_Params]
;--------------------------------------
; Old Keyword Cleanup
;--------------------------------------
HKR, Ndi\Params\DirectEnable
HKR, Ndi\Params\DuplexMode
HKR, Ndi\Params\EarlyReceive
HKR, Ndi\Params\EarlyTransmit
HKR, Ndi\Params\InterruptStyle
HKR, Ndi\Params\SocketNumber
HKR, Ndi\Params\MODE
HKR, Ndi\Params\Mode
HKR, Ndi\Params\LineMode
HKR, Ndi\Params\LineSpeed

[Delreg_NICNT_Params]
;--------------------------------------
; Old Keyword Cleanup
;--------------------------------------
HKR, Ndi\Params\EarlyReceive
HKR, Ndi\Params\EarlyTransmit
HKR, Ndi\Params\LEDEnabled
HKR, Ndi\Params\MODE
HKR, Ndi\Params\Mode
HKR, Ndi\Params\LineMode
HKR, Ndi\Params\LineSpeed
