; ** Copyright 2010, TP-LINK TECHNOLOGIES CO., LTD.
;
; TP-LINK  Gigabit  PCI  Network  Adapter
;
;; .this release is primarily for motherboard OEM for WHQL test.

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %Realtek%                               
CatalogFile.NT    = netrtl.cat
DriverVer      = 07/19/2006,5.649.0615.2006

[Manufacturer]
%Realtek%   = Realtek, NT.5.1, NTamd64.5.1, NT.6.0, NTamd64.6.0, NT.6.1, NTamd64.6.1

[ControlFlags]
ExcludeFromSelect = PCI\VEN_10EC&DEV_8139
ExcludeFromSelect = PCI\VEN_10EC&DEV_8169
ExcludeFromSelect = PCI\VEN_10EC&DEV_8167

[Realtek]
; DisplayName            Section            DeviceID
; -----------            -------            --------
;%RTL8169.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8169
;%RTL8169.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8167
;%RTL8169.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8169&SUBSYS_816910EC
;%RTL8169.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8167&SUBSYS_816710EC

[Realtek.NT.5.1]; This section will only be installed by Windows XP
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8169
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167
%RTL8139.DeviceDesc%    = RTL8139x.ndi,     PCI\VEN_10EC&DEV_8139&REV_10
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8169&SUBSYS_816910EC
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_816710EC
%RTL8139.DeviceDesc%    = RTL8139x.ndi,     PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_10
%RTL8139P.DeviceDesc%   = RTL8139Px.ndi,    PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_20
;OEM IDs for GBE(8167)
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_009A1025;Acer
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_009B1025;Acer
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1077147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_107B147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_107D147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_107E147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1080147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_108A147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_108B147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_180A147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_240B147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_240C147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_240E147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_13451043;ASUS
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_820D1043;ASUS
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_81671019;ECS
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_90381695;Epox
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60041509;FIC
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60081509;FIC
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_601D1509;FIC
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C4C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C82105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C84105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C85105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C97105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C98105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C99105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9A105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9F105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CC5105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CCB105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF0105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_10D01734;FSC
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_2A37103C;HP
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_3023103C;HP
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_100717AA;Lenovo
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_100A17AA;Lenovo
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_383617AA;Lenovo
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_251C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_258C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_263C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_277C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_279C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_280C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_281C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_300C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_305C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_312C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_381C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_88031033;NEC
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_C0191631;RT_QTA
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_008317C0;Wistron
;OEM IDs for GBE(8169)
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00361025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006A1025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006E1025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00711025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00731025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_007D1025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_007E1025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_007F1025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00791025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_009A1025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_009B1025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_009F1025 ;acer
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_102D147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_102F147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1032147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1039147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1045147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_105F147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106C147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106D147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106E147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_106F147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_180A147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2208147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_240A147B ;ABIT
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60201915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60211915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60221915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60231915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60241915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_46051961 ;AMOI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F7A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F8A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F9A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03FAA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0405A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0406A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_040CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_041CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0449A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_044AA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045BA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045EA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045FA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0460A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0461A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0462A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_046DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_046EA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0477A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049EA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049FA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A0A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A1A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A2A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CAA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CBA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CCA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CDA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0526A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0528A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_052AA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0542A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0543A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054BA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054FA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0563A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_057CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0583A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0589A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058AA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0600A0A0 ;AOpen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0601A0A0 ;AOpen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0602A0A0 ;AOpen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0604A0A0 ;AOpen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_060EA0A0 ;AOpen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_202F161F ;Arima
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10A61043 ;ASUS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_11E51043 ;ASUS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_11F51043 ;ASUS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_81CB104D ;ASUS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0121631 ;ASUS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_23031565 ;Biostar
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_23041565 ;Biostar
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_F446270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2793270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_272B270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_273B270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_F644270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_7842270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_7860270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00031854 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02951558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02971558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03751558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04501558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04511558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04521558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04701558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04761558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04801558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A01558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05051558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05061558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05071558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05081558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05091558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05201558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05601558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05701558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05711558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05721558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_06601558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08051558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08061558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08071558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08081558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08091558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_47011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_47021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_54011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_54051558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_001214C0 ;Compal
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_001714C0 ;Compal
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3085103C ;Compal
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_FF001179 ;Compal
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_100A15BD ;DFI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F271019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F471019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F521019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F561019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F661019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F671019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B111019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18651019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18731019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18741019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18531019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18031019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B081019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B101019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_81691019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_90221695 ;Epox
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_28211509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60011509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60021509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60031509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60041509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60051509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60061509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60071509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60081509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60091509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60101509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60111509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60121509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60131509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60141509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60151509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60161509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60171509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60181509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60191509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60201509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60211509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60221509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60231509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60241509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60251509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60261509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60271509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60281509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60291509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_602F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80011509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80021509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80031509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80041509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80051509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80061509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80071509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80081509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80091509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80101509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80111509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80121509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80131509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80141509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80151509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80161509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80171509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80181509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80191509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_801F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80201509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80211509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80221509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80231509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80241509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80251509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80261509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80271509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80281509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80291509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_802F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92171509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92181509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_921F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92201509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92221509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92231509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92261509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92451509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92461509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92471509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92481509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92491509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92511509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92521509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92671509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92691509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92701509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92731509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92741509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92751509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92761509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92771509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92781509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92791509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C06105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C07105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C08105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C09105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C10105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C11105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C12105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C13105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C14105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C15105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C16105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C17105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C18105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C19105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C20105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C21105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C22105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C23105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C24105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C25105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C26105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C27105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C28105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C29105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C30105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C31105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C32105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C33105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C34105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C35105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C36105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C37105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C38105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C39105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C41105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C42105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C43105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C44105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C45105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C46105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C47105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C48105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C49105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C51105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C52105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C53105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C54105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C55105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C56105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C57105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C58105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C59105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C60105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C61105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C62105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C63105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C64105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C65105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C69105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C6F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C70105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C71105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C72105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C73105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C74105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C75105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C7E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C80105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C81105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C82105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C83105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C84105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C85105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C90105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C91105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C92105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C93105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C94105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C95105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C97105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C98105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C99105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C9F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA0105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA1105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA2105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA3105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA4105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA5105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA6105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA7105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA8105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA9105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAA105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAB105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAC105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAD105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAE105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAF105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC5105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC6105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC7105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC8105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CC9105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCA105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCB105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCC105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCD105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCE105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CCF105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF0105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF1105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF2105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF3105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF4105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF5105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF6105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF7105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF8105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CF9105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFA105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFB105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFC105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFD105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFE105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CFF105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10911734 ;FSC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0001458 ;GIGABYTE
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_FE001458 ;GIGABYTE
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_FE011458 ;GIGABYTE
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0091631 ;GIGABYTE
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020E103C ;HP
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2A17103C ;HP
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_301F103C ;HP
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3022103C ;HP
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3023103C ;HP
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3081103C ;HP
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_308F103C ;HP
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3091103C ;HP
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00071170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_000A1170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_000B1170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00201170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500417FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500517FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500617FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500D17FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10EC16F3 ;Jetway
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_811016F3 ;Jetway
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_383617AA ;Lenovo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80061854 ;LG
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80071854 ;LG
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80081854 ;LG
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80091854 ;LG
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800A1854 ;LG
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800B1854 ;LG
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800C1854 ;LG
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800D1854 ;LG
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800E1854 ;LG
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_800F1854 ;LG
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01241071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01711071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80171071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80501071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_83171071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80661071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C0081631 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C00A1631 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_003C1462 ;MS-7003
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006C1462 ;MS-7006
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_008C1462 ;MS-7008
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01611462 ;MS-1016
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_02411462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_028C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_033C1462 ;MS-7033
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_062C1462 ;MS-7062
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_094C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_097C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_101C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_108C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_11501462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_131C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_133C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_139C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_143C1462 ;MS-7143
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_151C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_166C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_173C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_176C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_177C1462 ;MS-7177
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_183C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_191C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_194C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_19601462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_204C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_208C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_209C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_210C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_211C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_215C1462 ;MS-7215
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_222C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_223C1462 ;MS-7223
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_229C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_232C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_235C1462 ;MS-7235
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_236C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_240C1462 ;MS-7240
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_241C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_242C1462 ;MS-7242
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_248C1462 ;MS-7248
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_251C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_254C1462 ;MS-7254
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_258C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_267C1462 ;MS-7254
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_275C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_279C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_308C1462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_702C1462 ;MS-6702
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_72111462 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_728C1462 ;MS-6728
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_758C1462 ;MS-6758
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_771C1462 ;MS-6771
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_788C1462 ;MS-6788
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_799C1462 ;MS-6799
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_D0071631 ;MSI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_D0081631 ;MS-7168
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E00F1631 ;MS-7069
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0111631 ;MS-7069
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_82B61033 ;NEC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_833810F7 ;Panasonic
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0746152D ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0729152D ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0730152D ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058A17FF ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058B17FF ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_107D1734 ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C0111631 ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C00B1631 ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C00D1631 ;RT_QTA
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_100817AA ;Lenovo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_100A17AA ;Lenovo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3BE617AA ;Lenovo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_31558452 ;Topstar
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_5003148C ;TUL
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020B14FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020E14FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020F14FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_021214FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_107C1734 ;Uniwill_FjSi
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10AC1734 ;Uniwill_FjSi
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10B01734 ;Uniwill_FjSi
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_51081584 ;Uniwill
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_97101584 ;Uniwill
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_003317C0 ;Wistron
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_105317C0 ;Wistron
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_109417C0 ;Wistron

[Realtek.NTamd64.5.1]; This section will only be installed by Windows XP 64-bit
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8169
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167
%RTL8139.DeviceDesc%    = RTL8139a.ndi,     PCI\VEN_10EC&DEV_8139&REV_10
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8169&SUBSYS_816910EC
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_816710EC
%RTL8139.DeviceDesc%    = RTL8139a.ndi,     PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_10
%RTL8139P.DeviceDesc%   = RTL8139Pa.ndi,    PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_20
;OEM GBE IDs for x64(8167)
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_009A1025;Acer
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_009B1025;Acer
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1077147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_107B147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_107D147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_107E147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_1080147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_108A147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_108B147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_180A147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_240B147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_240E147B;ABIT
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_13451043;ASUS
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_820D1043;ASUS
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_81671019;ECS
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_90381695;Epox
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60041509;FIC
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_60081509;FIC
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_601D1509;FIC
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C4C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CC5105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C7E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C82105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C84105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C85105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C97105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C98105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C99105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9A105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9B105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9C105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9D105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9E105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0C9F105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CCB105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_0CF0105B;Foxconn
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_10D01734;FSC
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_2A37103C;HP
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_3023103C;HP
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_100717AA;Lenovo
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_100A17AA;Lenovo
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_383617AA;Lenovo
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_251C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_258C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_263C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_277C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_279C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_281C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_280C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_300C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_305C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_312C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_318C1462;MSI
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_88031033;NEC
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_C0191631;RT_QTA
%RTL8169.DeviceDesc%    = RTL8169a.ndi,     PCI\VEN_10EC&DEV_8167&SUBSYS_008317C0;Wistron
;OEM GBE IDs for x64(8169)
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_1045147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_1039147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_1032147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_102D147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_105F147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_106C147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_106D147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_106E147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_106F147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_180A147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_2208147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_240A147B ;ABIT
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_00791025 ;acer
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_007D1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_009A1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_009B1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_009F1025 ;acer
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_816917F2 ;Albatron
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0542A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0563A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0571A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_057CA0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0583A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0589A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_058AA0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0600A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0601A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0602A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0604A0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_060EA0A0 ;AOpen
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_FF001179 ;Asrock
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_10A61043 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_11E51043 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_11F51043 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_81631043 ;ASUS
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_01201558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_02971558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_04501558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_04511558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_04521558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_04531558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_04541558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_05601558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_05701558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_05711558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_05721558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_09001558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_09011558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_09021558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_09031558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_09041558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_47011558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_54021558 ;Clevo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_001214CO ;Compal
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_002014CO ;Compal
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_100A15BD ;DFI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0F661019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0F671019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_81691019 ;ECS
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_90221695 ;EPoX
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_801A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_801B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_801C1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_801D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_801E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_801F1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_92501509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_92551509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_92561509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_92591509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_925A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_925D1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_92611509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_92671509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_92691509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_926E1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_927A1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_927B1509 ;FIC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C21105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C22105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C23105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C24105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C25105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C26105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C27105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C2A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C2B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C2C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C2D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C2E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C2F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C32105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C33105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C34105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C35105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C36105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C37105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C39105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C3A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C44105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C54105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C58105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C64105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C69105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C6B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C6C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C6D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C6E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C6F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C7B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C7C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C7D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C7E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C7F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C81105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C82105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C83105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C84105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C85105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C8E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C90105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C91105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C92105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C93105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C94105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C95105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C97105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C98105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C99105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C9A105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C9B105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C9C105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C9D105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C9E105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0C9F105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CA0105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CA1105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CA2105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CA3105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CA4105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CA5105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CA6105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CA7105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CA8105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CA9105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CAA105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CAB105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CAC105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CAD105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CAE105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CAF105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CC0105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CC1105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CC2105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CC3105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CC4105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CC5105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CC6105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CC7105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CC8105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CC9105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CCA105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CCB105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CCC105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CCD105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CCE105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CCF105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CF0105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CF1105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CF2105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CF3105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CF4105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CF5105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CF6105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CF7105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CF8105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CF9105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CFA105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CFB105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CFC105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CFD105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CFE105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_0CFF105B ;Foxconn
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_10911734 ;FSC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_10931734 ;FSC
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_FE001458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_FE011458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_E0001458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_66661458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_32001458 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_E0091631 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_70031631 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_E0001940 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_03001014 ;GIGABYTE
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_301F103C ;HP
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_3022103C ;HP
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_3023103C ;HP
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_383617AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_3BE617AA ;Lenovo
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_80061854 ;LG
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_80071854 ;LG
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_80081854 ;LG
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_80091854 ;LG
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800A1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800B1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800C1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800D1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800E1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_800F1854 ;LG
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_01611462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_02411462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_028C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_033C1462 ;MS-7033
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_058C1462 ;MS-7058
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_062C1462 ;MS-7062
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_094C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_097C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_101C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_108C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_131C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_133C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_139C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_140C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_143C1462 ;MS-7143
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_151C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_166C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_173C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_176C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_177C1462 ;MS-7177
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_183C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_191C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_194C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_204C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_208C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_209C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_210C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_211C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_215C1462 ;MS-7215
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_222C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_223C1462 ;MS-7223
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_229C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_232C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_235C1462 ;MS-7235
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_236C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_240C1462 ;MS-7240
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_241C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_242C1462 ;MS-7242
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_248C1462 ;MS-7428
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_251C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_254C1462 ;MS-7254
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_258C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_267C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_275C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_279C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_308C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_702C1462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_72111462 ;MSI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_728C1462 ;MS-6728
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_E00F1631 ;NECCI
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_82971033 ;NECP
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_826E1033 ;NECP
%RTL8169.DeviceDesc%  = RTL8169a.ndi,  PCI\VEN_10EC&DEV_8169&SUBSYS_10921734 ;Wistron
[Realtek.NT.6.0]
;
[Realtek.NTamd64.6.0]
;
[Realtek.NT.6.1]
;
[Realtek.NTamd64.6.1]
;

;;****************************************************************************
;; Windows 98/ME
;;****************************************************************************
[rtl8139.ndi]
DriverVer       = 07/19/2006,649
AddReg          = rtl8139.id.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
CopyFiles       = Rtlnic.CopyFiles9x

[rtl8139P.ndi]
DriverVer       = 07/19/2006,649
AddReg          = rtl8139.id.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
CopyFiles       = Rtlnic.CopyFiles9x

[rtl8169.ndi]
DriverVer       = 07/19/2006,649
AddReg          = rtl8169.id.reg, RTLnic.all.reg, RTL8169.common.reg
CopyFiles       = Rtlnic.CopyFiles9x

[RTL8139_TOS.ndi]
DriverVer       = 07/19/2006,649
AddReg          = rtl8139.id.reg, RTLnic.all.reg, RTL8139TOS.common.reg
CopyFiles       = Rtlnic.CopyFiles9x

[rtl8136.ndi]
DriverVer       = 07/19/2006,649
AddReg          = rtl8136.id.reg, RTLnic.all.reg, RTL8136.common.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;; Windows 2000
;;****************************************************************************
[RTL8139.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8139P.ndi.NT]
DelReg          = CpPreParams.DelReg
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL39.common.reg, RTL39p.only.reg, RTL39p.w2k.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139P.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8169.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL8169.common.reg, RTL8169.W2K.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8169.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8139_TOS.ndi.NT]
DelReg          = PreParams.DelReg           
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL8139TOS.common.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139_TOS.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8136.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL8136.common.reg, RTL8136.W2K.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8136.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[Rtlnic.CopyFiles]
Rtnic.sys,,,2

[Rtlnic.CopyFiles9x]
Rtnic.sys,,,2

;;****************************************************************************
;; Windows XP
;;****************************************************************************
[RTL8139x.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8139x.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

[RTL8139_TOSx.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL8139TOS.common.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8139_TOSx.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

[RTL8139Px.ndi.NT]
DelReg          = CpPreParams.DelReg
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL39.common.reg, RTL39p.only.reg, RTL39p.w2k.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8139Px.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

[RTL8169x.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL8169.common.reg, RTL8169.W2K.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8169x.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

[RTL8136x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL8136.common.reg, RTL8136.W2K.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8136x.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

[Rtlnic.CopyFilesXP]
Rtnicxp.sys,,,2

;;****************************************************************************
;; Windows XP 64-bit
;;****************************************************************************
[RTL8139a.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8023x64.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8139a.ndi.NT.Services]
AddService = RTL8023x64, 2, rtsntx64.Service, common.EventLog

[RTL8139Pa.ndi.NT]
DelReg          = CpPreParams.DelReg
AddReg          = RTL8023x64.reg, RTLnic.all.reg, RTL39.common.reg, RTL39p.only.reg, RTL39p.w2k.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8139Pa.ndi.NT.Services]
AddService = RTL8023x64, 2, rtsntx64.Service, common.EventLog

[RTL8169a.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8023x64.reg, RTLnic.all.reg, RTL8169.common.reg, RTL8169.W2K.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8169a.ndi.NT.Services]
AddService = RTL8023x64, 2, rtsntx64.Service, common.EventLog

[RTL8136a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8023x64.reg, RTLnic.all.reg, RTL8136.common.reg, RTL8136.W2K.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8136a.ndi.NT.Services]
AddService = RTL8023x64, 2, rtsntx64.Service, common.EventLog

[Rtlnic.CopyFilesX64]
Rtnic64.sys,,,2

;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[rtl8139.id.reg]
HKR,,                 MediaType,          0,    1
HKR,,                 AdapterType,        0,    5
HKR,,                 BusType,            0,    5
HKR,,                 DevLoader,          0,    "*ndis"
HKR,,                 DeviceVxDs,         0,    "Rtnic.sys"
HKR,,                 EnumPropPages,      0,    "netdi.dll,EnumPropPages"
HKR,NDIS,             MajorNdisVersion,   1,    03
HKR,NDIS,             MinorNdisVersion,   1,    0A
HKR,NDIS,             LogDriverName,      0,    "RTL8023"
HKR,Ndi,              DeviceID,           0,    "PCI\VEN_10EC&DEV_8139"
HKR,Ndi\Install,      ndis3,              0,    "rtl139.ndis5"
HKR,Ndi\Interfaces,   DefLower,            ,    "ethernet"
HKR,Ndi\Interfaces,   LowerRange,          ,    "ethernet"
HKR,Ndi\Interfaces,   DefUpper,            ,    "ndis3"
HKR,Ndi\Interfaces,   UpperRange,          ,    "ndis3"

[rtl8169.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtnic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTL8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8169"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

[rtl8136.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtnic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTL8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8136"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

;;****************************************************************************
;; common parameters
;;****************************************************************************
[RTLnic.all.reg]
HKR,Ndi\params\NetworkAddress,  ParamDesc,      0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,  type,           0, "edit"
HKR,Ndi\params\NetworkAddress,  default,        0, "000000000000"
HKR,Ndi\params\NetworkAddress,  LimitText,      0, "12"
HKR,Ndi\params\NetworkAddress,  UpperCase,      0, "1"
HKR,Ndi\params\NetworkAddress,  Optional,       0, "1"

[RTL39.common.reg]
HKR,Ndi\params\DuplexMode,        ParamDesc,   0, %SpeedDuplexMode%
HKR,Ndi\params\DuplexMode,        type,        0, "enum"
HKR,Ndi\params\DuplexMode,        default,     0, "1"
HKR,Ndi\params\DuplexMode\enum,   1,           0, %auto_nego%
HKR,Ndi\params\DuplexMode\enum,   2,           0, %sd10half%
HKR,Ndi\params\DuplexMode\enum,   3,           0, %sd10full%
HKR,Ndi\params\DuplexMode\enum,   4,           0, %sd100half%
HKR,Ndi\params\DuplexMode\enum,   5,           0, %sd100full%

HKR,Ndi\params\OptimalPerf,      ParamDesc,  0, %OptimalPerf%
HKR,Ndi\params\OptimalPerf,      default,    0, "0"
HKR,Ndi\params\OptimalPerf,      type,       0, "enum"
HKR,Ndi\params\OptimalPerf\enum, "1",        0, "Enable"
HKR,Ndi\params\OptimalPerf\enum, "0",        0, "Disable"

HKR,Ndi\params\WakeUpFrame,     ParamDesc,      0, %WOLCapability%
HKR,Ndi\params\WakeUpFrame,     default,        0, "1"
HKR,Ndi\params\WakeUpFrame,     type,           0, "enum"
HKR,Ndi\params\WakeUpFrame\enum,"0",            0, "Disable"
HKR,Ndi\params\WakeUpFrame\enum,"1",            0, "Enable"
HKR,,WakeUpFrame, 0, "1"

HKR,Ndi\params\LinkUp,           ParamDesc, 0, "WakeUp on Link Change"
HKR,Ndi\params\LinkUp,           default,   0, "0"
HKR,Ndi\params\LinkUp,           type,      0, "enum"
HKR,Ndi\params\LinkUp\enum,      "1",       0, "Enable"
HKR,Ndi\params\LinkUp\enum,      "0",       0, "Disable"

HKR,Ndi\params\EnableLDPS,       ParamDesc, 0, "Link Down Power Saving"
HKR,Ndi\params\EnableLDPS,       default,   0, "0"
HKR,Ndi\params\EnableLDPS,       type,      0, "enum"
HKR,Ndi\params\EnableLDPS\enum,  "1",       0, "Enable"
HKR,Ndi\params\EnableLDPS\enum,  "0",       0, "Disable"

[RTL39.only.reg]
HKR,Ndi\params\RxBufLen,         ParamDesc, 0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,         type,      0, "enum"
HKR,Ndi\params\RxBufLen,         default,   0, "3"
HKR,Ndi\params\RxBufLen\enum,    "0",       0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,    "1",       0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,    "2",       0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,    "3",       0, "64K bytes"

HKR,Ndi\params\RTPME,            ParamDesc, 0, "WakeUp using APM Mode"
HKR,Ndi\params\RTPME,            default,   0, "0"
HKR,Ndi\params\RTPME,            type,      0, "enum"
HKR,Ndi\params\RTPME\enum,       "1",       0, "Enable"
HKR,Ndi\params\RTPME\enum,       "0",       0, "Disable"

[RTL39p.only.reg]
HKR,Ndi\Params\NumCoalesce,       ParamDesc,  0, "Number of Tx Coalesce Buffer"
HKR,Ndi\Params\NumCoalesce,       Type,       0, "int"
HKR,Ndi\Params\NumCoalesce,       Default,    0, "16"
HKR,Ndi\Params\NumCoalesce,       Min,        0, "0"
HKR,Ndi\Params\NumCoalesce,       Max,        0, "32"
HKR,Ndi\Params\NumCoalesce,       Step,       0, "1"
HKR,Ndi\Params\NumCoalesce,       Base,       0, "10"

[PreParams.DelReg]
HKR,Ndi\Params\PME
HKR,,PME
HKR,Ndi\Params\EarlyTxThreshold
HKR,,EarlyTxThreshold

[CpPreParams.DelReg]
HKR,Ndi\Params\PME
HKR,,PME
HKR,Ndi\Params\RTPME
HKR,,RTPME
HKR,Ndi\Params\RxBufLen
HKR,,RxBufLen
HKR,Ndi\Params\EarlyTxThreshold
HKR,,EarlyTxThreshold

[GigPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid
HKR,Ndi\Params\CksOffload
HKR,,CksOffload
HKR,Ndi\Params\Largesend
HKR,,Largesend

[TsPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid

[RTL39p.w2k.reg]
HKR,Ndi\params\Offload,           ParamDesc,  0, "Task Offload"
HKR,Ndi\params\Offload,           default,    0, "1"
HKR,Ndi\params\Offload,           type,       0, "enum"
HKR,Ndi\params\Offload\enum,      "0",        0, "All Disable"
HKR,Ndi\params\Offload\enum,      "1",        0, "Checksum"
HKR,Ndi\params\Offload\enum,      "2",        0, "Chksum & TCP_Segment"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

[RTL8139TOS.common.reg]
HKR,Ndi\params\RxBufLen,          ParamDesc,  0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,          type,       0, "enum"
HKR,Ndi\params\RxBufLen,          default,    0, "3"
HKR,Ndi\params\RxBufLen\enum,     "0",        0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,     "1",        0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,     "2",        0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,     "3",        0, "64K bytes"

HKR,Ndi\params\LinkUp,            ParamDesc,  0, "WakeUp on Link Change"
HKR,Ndi\params\LinkUp,            default,    0, "0"
HKR,Ndi\params\LinkUp,            type,       0, "enum"
HKR,Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR,Ndi\params\LinkUp\enum,       "0",        0, "Disable"

HKR,Ndi\params\WakeUpFrame,       ParamDesc,  0, "WakeUp on ARP/PING"         
HKR,Ndi\params\WakeUpFrame,       default,    0, "1"                          
HKR,Ndi\params\WakeUpFrame,       type,       0, "enum"                       
HKR,Ndi\params\WakeUpFrame\enum,  "1",        0, "Enable"                     
HKR,Ndi\params\WakeUpFrame\enum,  "0",        0, "Disable"                    

HKR,Ndi\params\RTPME,             ParamDesc,  0, "WakeUp using APM Mode"      
HKR,Ndi\params\RTPME,             default,    0, "0"                          
HKR,Ndi\params\RTPME,             type,       0, "enum"                      
HKR,Ndi\params\RTPME\enum,        "1",        0, "Enable"                     
HKR,Ndi\params\RTPME\enum,        "0",        0, "Disable"                   

HKR,Ndi\params\EnableLDPS,        ParamDesc,  0, "Link Down Power Saving"
HKR,Ndi\params\EnableLDPS,        default,    0, "1"
HKR,Ndi\params\EnableLDPS,        type,       0, "enum"
HKR,Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"
HKR,Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"

HKR,Ndi\params\TxMaxDMABurst,     ParamDesc,  0, "Transmit DMA burst size"  
HKR,Ndi\params\TxMaxDMABurst,     type,       0, "enum"                           
HKR,Ndi\params\TxMaxDMABurst,     default,    0, "6"                           
HKR,Ndi\params\TxMaxDMABurst\enum,0,          0, "16 bytes"                  
HKR,Ndi\params\TxMaxDMABurst\enum,1,          0, "32 bytes"        
HKR,Ndi\params\TxMaxDMABurst\enum,2,          0, "64 bytes"         
HKR,Ndi\params\TxMaxDMABurst\enum,3,          0, "128 bytes"         
HKR,Ndi\params\TxMaxDMABurst\enum,4,          0, "256 bytes"        
HKR,Ndi\params\TxMaxDMABurst\enum,5,          0, "512 bytes"            
HKR,Ndi\params\TxMaxDMABurst\enum,6,          0, "1024 bytes"             
HKR,Ndi\params\TxMaxDMABurst\enum,7,          0, "2048 bytes"             

HKR,Ndi\params\RxMaxDMABurst,     ParamDesc,  0, "Receive DMA burst size"  
HKR,Ndi\params\RxMaxDMABurst,     type,       0, "enum"
HKR,Ndi\params\RxMaxDMABurst,     default,    0, "6"                      
HKR,Ndi\params\RxMaxDMABurst\enum,0,          0, "16 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,1,          0, "32 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum,2,          0, "64 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum,3,          0, "128 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,4,          0, "256 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,5,          0, "512 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,6,          0, "1024 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,7,          0, "unlimitted"               

HKR,Ndi\params\EarlyRxThreshold,  ParamDesc,  0, "Receive FIFO threshold"   
HKR,Ndi\params\EarlyRxThreshold,  type,       0, "enum"
HKR,Ndi\params\EarlyRxThreshold,  default,    0, "2"
HKR,Ndi\params\EarlyRxThreshold\enum,0,       0, "16 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,1,       0, "32 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,2,       0, "64 bytes"
HKR,Ndi\params\EarlyRxThreshold\enum,3,       0, "128 bytes"
HKR,Ndi\params\EarlyRxThreshold\enum,4,       0, "256 bytes"
HKR,Ndi\params\EarlyRxThreshold\enum,5,       0, "512 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,6,       0, "1024 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,7,       0, "No threshold"

HKR,,EnableLDPS,        0,   "1"
HKR,,WakeUpFrame,       0,   "1"          
HKR,,RTPME,             0,   "0"         
HKR,,LinkUp,            0,   "0"
HKR,,RxBufLen,          0,   "3"
HKR,,EarlyRxThreshold,  0,   "2"
HKR,,RxMaxDMABurst,     0,   "6"
HKR,,TxMaxDMABurst,     0,   "6" 

[RTL8169.common.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR, Ndi\params\DuplexMode\enum,  6,          0, %sd1000full%

;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"

;HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
;HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"

HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, "Disable"
HKR,Ndi\params\Jumboframe\enum,   "1",        0, "2KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "2",        0, "3KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "3",        0, "4KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "4",        0, "5KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "5",        0, "6KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "6",        0, "7KB MTU"

HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "1"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, "Disable"
HKR,Ndi\params\FlowControl\enum, "1",        0, "Enable"
HKR,,FlowControl,0,"1" 

HKR,,SuperSwitch,0,"0"

;HKR,Ndi\params\S5WakeOnLan,      ParamDesc,  0, %S5Wake-On-Lan%
;HKR,Ndi\params\S5WakeOnLan,      default,    0, "1"
;HKR,Ndi\params\S5WakeOnLan,      type,       0, "enum"
;HKR,Ndi\params\S5WakeOnLan\enum, "0",        0, "Disable"
;HKR,Ndi\params\S5WakeOnLan\enum, "1",        0, "Enable"

;HKR,Ndi\params\AutoSpeedDown,         ParamDesc,  0, %AutoSpeedDown%
;HKR,Ndi\params\AutoSpeedDown,         default,    0, "1"
;HKR,Ndi\params\AutoSpeedDown,         type,       0, "enum"
;HKR,Ndi\params\AutoSpeedDown\enum,    "1",        0, "Enable"
;HKR,Ndi\params\AutoSpeedDown\enum,    "0",        0, "Disable"

[RTL8136.common.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%

;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"

;HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
;HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"

HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, "Disable"
HKR,Ndi\params\Jumboframe\enum,   "1",        0, "2KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "2",        0, "3KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "3",        0, "4KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "4",        0, "5KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "5",        0, "6KB MTU"
;HKR,Ndi\params\Jumboframe\enum,   "6",        0, "7KB MTU"

HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "1"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, "Disable"
HKR,Ndi\params\FlowControl\enum, "1",        0, "Enable"
HKR,,FlowControl,0,"1" 

[RTL8169.W2K.reg]
HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, "Disable"
HKR,Ndi\params\CksOffload\enum,   "1",        0, "Tx/Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "3",        0, "Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "4",        0, "Tx Checksum"
HKR,,CksOffload,0,"1"

HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "1"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "1",        0, "Enable"
HKR,Ndi\params\Largesend\enum,    "0",        0, "Disable"
HKR,,Largesend,0,"1"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

;HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
;HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
;HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
;HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
;HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
;HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
;HKR,Ndi\Params\RegVlanid,   Base,       0, "10"

;HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
;HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
;HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "256"
;HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
;HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "512"
;HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
;HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"

[RTL8136.W2K.reg]
HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, "Disable"
HKR,Ndi\params\CksOffload\enum,   "1",        0, "Tx/Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "3",        0, "Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "4",        0, "Tx Checksum"

HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "1"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "1",        0, "Enable"
HKR,Ndi\params\Largesend\enum,    "0",        0, "Disable"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

;HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
;HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
;HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
;HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
;HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
;HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
;HKR,Ndi\Params\RegVlanid,   Base,       0, "10"

;HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
;HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
;HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "256"
;HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
;HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "512"
;HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
;HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"

HKR,,CksOffload,0,"1" 
HKR,,Largesend,0,"1" 

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTL8023.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8023"

[rtsnt.Service]
DisplayName     = %Rtlnic.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtnic.sys
LoadOrderGroup  = NDIS

[RTL8023xp.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8023xp"

[rtsntxp.Service]
DisplayName     = %Rtlnicxp.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtnicxp.sys
LoadOrderGroup  = NDIS

[RTL8023x64.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8023x64"

[rtsntx64.Service]
DisplayName     = %Rtlnicx64.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtnic64.sys
LoadOrderGroup  = NDIS

[common.EventLog]
Addreg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
Rtlnic.CopyFiles           = 12
Rtlnic.CopyFilesXP         = 12
Rtlnic.CopyFilesX64        = 12
Rtlnic.CopyFiles9x         = 11
DefaultDestDir             = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
Rtnic.sys       = 1
Rtnicxp.sys     = 1
Rtnic64.sys     = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek                 = "TP-LINK"
VLanTagging             = "802.1Q/1p VLAN Tagging"
;VLanID                 = "802.1Q VLAN ID"
ChecksumOffload         = "Offload Checksum"
LargesendOffload        = "Offload TCP_LargeSend"
SpeedDuplexMode         = "Link Speed/Duplex Mode"
auto_nego               = "Auto Negotiation"
sd10half                = "10Mbps/Half Duplex"
sd10full                = "10Mbps/Full Duplex"
sd100half               = "100Mbps/Half Duplex"
sd100full               = "100Mbps/Full Duplex"
sd1000full              = "1000Mbps/Full Duplex"
NetworkAddress          = "Network Address"
JumboFrame              = "Jumbo Frame"
;TxDescNumber           = "Number of Tx Descriptor"
;RxDescNumber           = "Number of Rx Descriptor"
;TxHPQDescNumber        = "Number of High Priority Tx Descriptor"
WOLCapability           = "WakeUp on ARP/PING"
WOLLinkChange           = "WakeUp on Link Change"
LDPSCapability          = "Link Down Power Saving"
OptimalPerf             = "Optimal Performance"
FlowControl             = "Flow Control"
AutoSpeedDown           = "Auto Speed Down"
S5Wake-On-Lan           = "S5 Wake-On-Lan"

;;Source disk name
DISKNAME = "TP-LINK TG-3269 Series Gigabit Ethernet Adapter Driver Diskette"

RTL8169.DeviceDesc        = "TP-LINK  Gigabit  PCI  Network  Adapter"
RTL8139.DeviceDesc        = "TP-LINK TF-3239 Fast Ethernet NIC"
RTL8139P.DeviceDesc       = "TP-LINK TF-3239 Fast Ethernet NIC"
RTL8139Panasonic.DeviceDesc = "(MOBILE ASSIST)Realtek RTL8139/810x Family Fast Ethernet NIC"

;;NT service name
Rtlnic.Service.DispName    = "TP-LINK 10/100/1000 NIC Family all in one NDIS NT Driver"
Rtlnicxp.Service.DispName    = "TP-LINK 10/100/1000 NIC Family all in one NDIS XP Driver"
Rtlnicx64.Service.DispName    = "TP-LINK 10/100/1000 NIC Family all in one NDIS XP(x64) Driver"

