; m4cxvst64.inf created 12-Jan-2007
;
; D-Link Gigabit Ethernet Adapter 
;
; (C)Copyright 2002-2007 Marvell(R).
; 
; All rights reserved.
;
; INF File for NDIS6.0 Miniport Driver for Windows Vista x64 M4CXVST64.sys v9.15.2.3

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider	= %D-Link%
CatalogFile	= m4cxvst64.CAT
DriverVer       = 01/12/2007, 9.15.2.3

[Manufacturer]
%D-Link%	= D-Link, NTamd64.6.0

[ControlFlags]

ExcludeFromSelect	= *


;-----------------------------------------------------------------------------
;
;       Windows 2000
;
;-----------------------------------------------------------------------------
[D-Link]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows XP
;
;-----------------------------------------------------------------------------
[D-Link.NT.5.1]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows Server 2003
;
;-----------------------------------------------------------------------------
[D-Link.NT.5.2]
;Empty section

;-----------------------------------------------------------------------------
;
;       Windows Vista
;
;-----------------------------------------------------------------------------

[D-Link.NTAMD64.6.0]
%Yukon-4001.DeviceDesc% = SLYuk2FibGig.ndi, PCI\VEN_1186&DEV_4001&SUBSYS_40011186
%Yukon-4346.DeviceDesc% = SLYuk2FibGig.ndi, PCI\VEN_1186&DEV_4346&SUBSYS_43461186
%Yukon-4B00.DeviceDesc% = SLYuk2CopGig.ndi, PCI\VEN_1186&DEV_4B00&SUBSYS_4B001186
%Yukon-4B01.DeviceDesc% = SLYukCopGig.ndi, PCI\VEN_1186&DEV_4B01&SUBSYS_4B011186
%Yukon-4B02.DeviceDesc% = SLYuk2FibGig.ndi, PCI\VEN_1186&DEV_4B02&SUBSYS_4B021186
%Yukon-4C00.DeviceDesc% = SLYukCopGig.ndi, PCI\VEN_1186&DEV_4C00&SUBSYS_4C001186


;-------------------------------------------------------------------------------
; (1)

[SLYuk2CopGig.ndi]
AddReg		= m4cxvst64.reg, m4cxvst64.common.params, m4cxvst64.YKVS_SL, m4cxvst64.GigFrSize.params, m4cxvst64.SLSpeedDuplex.params, m4cxvst64.SingleLink.params, m4cxvst64.TCPSegm.params, m4cxvst64.TxRxLE.params, m4cxvst64.WoLStd.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= m4cxvst64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2CopGig.ndi.Services]
AddService	= m4cxvst64, 2, m4cxvst64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (2)

[SLYuk2FibGig.ndi]
AddReg		= m4cxvst64.reg, m4cxvst64.common.params, m4cxvst64.YKVS_SL, m4cxvst64.GigFrSize.params, m4cxvst64.SingleLink.params, m4cxvst64.TxRxLE.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= m4cxvst64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYuk2FibGig.ndi.Services]
AddService	= m4cxvst64, 2, m4cxvst64.Service, common.EventLog


;-------------------------------------------------------------------------------
; (3)

[SLYukCopGig.ndi]
AddReg		= m4cxvst64.reg, m4cxvst64.common.params, m4cxvst64.YKVS_SL, m4cxvst64.GigFrSize.params, m4cxvst64.SLSpeedDuplex.params, m4cxvst64.SingleLink.params, m4cxvst64.TxRxBuff.params, m4cxvst64.WoLStd.params
Characteristics	= 0x84
BusType		= 5
CopyFiles	= m4cxvst64.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14	        ; NdisPhysicalMedium802_3

[SLYukCopGig.ndi.Services]
AddService	= m4cxvst64, 2, m4cxvst64.Service, common.EventLog



;-----------------------------------------------------------------------------
;
; General Driver Parameters
;
;-----------------------------------------------------------------------------
[m4cxvst64.common.params]


HKR, Ndi\Params\MessageLog,		ParamDesc,	0, %LogMsg%
HKR, Ndi\Params\MessageLog,		Type,		0, "enum"
HKR, Ndi\Params\MessageLog\enum,	"4",			0, %Non%
HKR, Ndi\Params\MessageLog\enum,	"3",			0, %Err%
HKR, Ndi\Params\MessageLog\enum,	"2",			0, %Wrn%
HKR, Ndi\Params\MessageLog\enum,	"1",			0, %Sta%
HKR, Ndi\Params\MessageLog\enum,	"0",			0, %All%
HKR, Ndi\Params\MessageLog,		Default,		0, "1"

HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, %IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, "enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, "3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, %TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, %UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\NetworkAddress,	ParamDesc,	0, %NetAddress%
HKR, Ndi\Params\NetworkAddress,	Type,		0, "edit"
HKR, Ndi\Params\NetworkAddress,	LimitText,	0, "18"
HKR, Ndi\Params\NetworkAddress,	UpperCase,	0, "1"
HKR, Ndi\Params\NetworkAddress,	Default,		0, ""
HKR, Ndi\Params\NetworkAddress,	Optional,		0, "1"

HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, %IntMod%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, "enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, "1"


HKR, Ndi\Params\FixedIntMod,	ParamDesc,	0, %MaxIrq%
HKR, Ndi\Params\FixedIntMod,	Type,		0, "int"
HKR, Ndi\Params\FixedIntMod,	Base,		0, "10"
HKR, Ndi\Params\FixedIntMod,	Min,			0, "1000"
HKR, Ndi\Params\FixedIntMod,	Max,			0, "30000"
HKR, Ndi\Params\FixedIntMod,	Step,		0, "1"
HKR, Ndi\Params\FixedIntMod,	Default,		0, "5000"

;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX buffers (V1 and V2)
;
;-----------------------------------------------------------------------------
[m4cxvst64.TxRxBuff.params]

HKR, Ndi\Params\*ReceiveBuffers,	ParamDesc,	0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,	Type,		0, "int"
HKR, Ndi\Params\*ReceiveBuffers,	Base,		0, "10"
HKR, Ndi\Params\*ReceiveBuffers,	Min,		0, "3"
HKR, Ndi\Params\*ReceiveBuffers,	Max,		0, "500"
HKR, Ndi\Params\*ReceiveBuffers,	Step,		0, "1"
HKR, Ndi\Params\*ReceiveBuffers,	Default,	0, "50"

HKR, Ndi\Params\*TransmitBuffers,ParamDesc,	0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,Type,		0, "int"
HKR, Ndi\Params\*TransmitBuffers,Base,		0, "10"
HKR, Ndi\Params\*TransmitBuffers,Min,		0, "4"
HKR, Ndi\Params\*TransmitBuffers,Max,		0, "200"
HKR, Ndi\Params\*TransmitBuffers,Step,		0, "1"
HKR, Ndi\Params\*TransmitBuffers,Default,	0, "50"
;-----------------------------------------------------------------------------
;
; Additional driver parameters for TX/RX LE (Y2)
;
;-----------------------------------------------------------------------------
[m4cxvst64.TxRxLE.params]

HKR, Ndi\Params\*ReceiveBuffers,	ParamDesc,	0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,	Type,		0, "int"
HKR, Ndi\Params\*ReceiveBuffers,	Base,		0, "10"
HKR, Ndi\Params\*ReceiveBuffers,	Min,		0, "256"
HKR, Ndi\Params\*ReceiveBuffers,	Max,		0, "512"
HKR, Ndi\Params\*ReceiveBuffers,	Step,		0, "128"
HKR, Ndi\Params\*ReceiveBuffers,	Default,	0, "256"

HKR, Ndi\Params\*TransmitBuffers,	ParamDesc,	0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,	Type,		0, "int"
HKR, Ndi\Params\*TransmitBuffers,	Base,		0, "10"
HKR, Ndi\Params\*TransmitBuffers,	Min,		0, "256"
HKR, Ndi\Params\*TransmitBuffers,	Max,		0, "512"
HKR, Ndi\Params\*TransmitBuffers,	Step,		0, "128"
HKR, Ndi\Params\*TransmitBuffers,	Default,	0, "256"
;-----------------------------------------------------------------------------
;
; Additional driver parameters for Maximum Frame Size (10/100/1000 chip)
;
;-----------------------------------------------------------------------------
[m4cxvst64.GigFrSize.params]

HKR, Ndi\params\*JumboPacket,	ParamDesc,	0, %JumboPacket%
HKR, Ndi\params\*JumboPacket,	Type,		0, "enum"
HKR, Ndi\params\*JumboPacket\enum,	"0",	0, "1514"
HKR, Ndi\params\*JumboPacket\enum,	"1",	0, "4088"
HKR, Ndi\params\*JumboPacket\enum,	"2",	0, "9014"
HKR, Ndi\params\*JumboPacket,	Default,	0, "1514"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for WakeOnLan
;
;-----------------------------------------------------------------------------
[m4cxvst64.WoLStd.params]

HKR, Ndi\Params\WakeUpModeCap_A,		ParamDesc,	0, %WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,		Type,		0, "enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"0",		0, %Non%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"25",		0, %MagicPacket%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"26",		0, %PatternMatch%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"27",		0, %MagPackPattMatch%
HKR, Ndi\Params\WakeUpModeCap_A\enum,	"28",		0, %LinkChange%
HKR, Ndi\Params\WakeUpModeCap_A,		Default,	0, "27"
;-----------------------------------------------------------------------------
;
; Additional driver parameters for TCP segmentation
;
;-----------------------------------------------------------------------------
[m4cxvst64.TcpSegm.params]

HKR, Ndi\Params\*LsoV1IPv4,			ParamDesc,	0, %LSOv1%
HKR, Ndi\Params\*LsoV1IPv4,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV1IPv4\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*LsoV1IPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*LsoV1IPv4,			Default,	0, "1"

;-----------------------------------------------------------------------------
;
; Additional Driver Parameters for Single Link Adapters
;
;-----------------------------------------------------------------------------
[m4cxvst64.SingleLink.params]

HKR, Ndi\Params\*PriorityVLANTag,		ParamDesc,	0, %PriorityVLAN%
HKR, Ndi\Params\*PriorityVLANTag,		Type,		0, "enum"
HKR, Ndi\Params\*PriorityVLANTag\enum,		"3",		0, %PrioVlanEna%
HKR, Ndi\Params\*PriorityVLANTag\enum,		"2",		0, %VlanEna%
HKR, Ndi\Params\*PriorityVLANTag\enum,		"1",		0, %PrioEna%
HKR, Ndi\Params\*PriorityVLANTag\enum,		"0",		0, %PrioVLANDis%
HKR, Ndi\Params\*PriorityVLANTag,		Default,	0, "0"

HKR, Ndi\Params\*FlowControl,		ParamDesc,	0, %FlowCtrl%
HKR, Ndi\Params\*FlowControl,		Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,		Default,	0, "3"

HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"

;-----------------------------------------------------------------------------
;
; Additional driver parameter to set the port speed and capabilities
;
;-----------------------------------------------------------------------------
[m4cxvst64.SLSpeedDuplex.params]

HKR,Ndi\Params\*SpeedDuplex,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,      Type,       0, "enum"
HKR,Ndi\Params\*SpeedDuplex,      Default,    0, "0"
HKR,Ndi\Params\*SpeedDuplex\enum, "0",        0, %Autosense%
HKR,Ndi\Params\*SpeedDuplex\enum, "1",        0, %10MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "2",        0, %10MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "3",        0, %100MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "4",        0, %100MFD%

HKR, Ndi\Params\*FlowControl,		ParamDesc,	0, %FlowCtrl%
HKR, Ndi\Params\*FlowControl,		Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,		Default,	0, "3"
;-----------------------------------------------------------------------------
;
; General Registry Entries
;
;-----------------------------------------------------------------------------
[m4cxvst64.reg]

HKR, Ndi\Interfaces, UpperRange,, "ndis5"

HKR, Ndi\Interfaces, LowerRange,, "ethernet"
HKR, Ndi, Service,, "m4cxvst64"

;-----------------------------------------------------------------------------
;
; Special Registry Entrries
;
;-----------------------------------------------------------------------------
[m4cxvst64.YKVS_SL]

;Key used by notify object
HKR,, YKVS,, "762751"

;-----------------------------------------------------------------------------
;
; Service
;
;-----------------------------------------------------------------------------
[m4cxvst64.Service]
DisplayName	= %m4cxvst64.DriverDesc%
ServiceType	= 1
StartType = 3
ErrorControl = 1
ServiceBinary  = %12%\m4cxvst64.sys
LoadOrderGroup = NDIS


;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.EventLog]
AddReg = common.AddEventLog.reg

;-----------------------------------------------------------------------------
;
;
;
;-----------------------------------------------------------------------------
[common.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\m4cxvst64.sys"
HKR,, TypesSupported,	0x00010001, 7


;-----------------------------------------------------------------------------
;
; Source Files
;
;-----------------------------------------------------------------------------
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
m4cxvst64.sys	= 1,,

[m4cxvst64.CopyFiles]
m4cxvst64.sys,,,2


;-----------------------------------------------------------------------------
;
; Destination Directories
;
;-----------------------------------------------------------------------------
[DestinationDirs]

DefaultDestDir = 12
m4cxvst64.CopyFiles	= 12

;-----------------------------------------------------------------------------
;
; Localizable Strings
;
;-----------------------------------------------------------------------------
[Strings]

D-Link = "D-Link Corporation"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Jumbo Packet"
ReceiveBuffers = "Receive Buffers"
TransmitBuffers = "Transmit Buffers"
IPChksumOffv4 = "IPv4 Checksum Offload"
TCPChksumOffv4 = "TCP Checksum Offload (IPv4)"
TCPChksumOffv6 = "TCP Checksum Offload (IPv6)"
UDPChksumOffv4 = "UDP Checksum Offload (IPv4)"
UDPChksumOffv6 = "UDP Checksum Offload (IPv6)"
LSOv1 = "Large Send Offload (IPv4)"
LSOv2IP4 = "Large Send Offload v2 (IPv4)"
LSOv2IP6 = "Large Send Offload v2 (IPv6)"
PriorityVLAN = "Priority & VLAN"
RSS = "Receive Side Scaling"
TXEna = "Tx Enabled"
RXEna = "Rx Enabled"
TXRXEna = "Tx & Rx Enabled"
PrioVlanDis = "Priority and VLAN Disabled"
PrioEna = "Priority Enabled"
VlanEna = "VLAN Enabled"
PrioVlanEna = "Priority & VLAN Enabled"

NetAddress   = "Network Address"
WakeUpCaps   = "Wake Up Capabilities"
IntMod = "Interrupt Moderation"
MaxIrq = "Max IRQ per Sec"
LogMsg = "Log Status Messages"
RLMT  = "RLMT Mode"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Preferred Port"
On = "On"
Off = "Off"
Enabled = "Enabled"
Disabled = "Disabled"
Non = "None"
Err = "Errors"
Wrn = "Warnings"
Sta = "Status Messages"
All = "All Messages"
A = "A"
B = "B"
Autosense = "Auto Negotiation"
10MHD = "10 Mbps Half Duplex"
10MFD = "10 Mbps Full Duplex"
100MHD = "100 Mbps Half Duplex"
100MFD = "100 Mbps Full Duplex"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Link Change"
SpeedDuplex = "Speed & Duplex"
FlowCtrl = "FlowControl"
WakeFromShut = "Wake From Shutdown"
BatSpeed = "BatterySpeedSettings"
SmartSpeed = "SmartSpeedDown"
MaxSpeed = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
;-----------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk Installation Disk"

Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


;-----------------------------------------------------------------------------

; Chinese (Taiwan)
[Strings.0404]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "特大包"
ReceiveBuffers = "接收緩衝"
TransmitBuffers = "傳輸緩衝"
IPChksumOffv4 = "卸載IPv4檢查和"
TCPChksumOffv4 = "卸載TCP檢查和(IPv4)"
TCPChksumOffv6 = "卸載TCP檢查和(IPv6)"
UDPChksumOffv4 = "卸載UDP檢查和(IPv4)"
UDPChksumOffv6 = "卸載UDP檢查和(IPv6)"
LSOv1 = "卸載超大發送(IPv4)"
LSOv2IP4 = "卸載超大發送v2(IPv4)"
LSOv2IP6 = "卸載超大發送v2(IPv6)"
PriorityVLAN = "802.1p優先權和VLAN"
RSS = "受端負載調節"
TXEna = "啟用Tx"
RXEna = "啟用Rx"
TXRXEna = "啟用Tx和Rx"
PrioVlanDis = "禁用優先權和VLAN"
PrioEna = "啟用優先權"
VlanEna = "啟用VLAN"
PrioVlanEna = "啟用優先權和VLAN"
NetAddress   = "網路位址"
WakeUpCaps   = "喚醒功能"
IntMod = "中斷模式"
MaxIrq = "最大 IRQ數量"
LogMsg = "日誌狀態訊息"
RLMT  = "RLMT 模式"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "偏好埠"
On = "開啟"
Off = "關閉"
Enabled = "啟用"
Disabled = "禁用"
Non = "無"
Err = "錯誤"
Wrn = "警告"
Sta = "狀態訊息"
All = "所有訊息"
A = "A"
B = "B"
Autosense = "自動感應"
10MHD = "10Mbps 半雙工"
10MFD = "10Mbps 全雙工"
100MHD = "100Mbps 半雙工"
100MFD = "100Mbps 全雙工"
MagicPacket = "Magic Packet喚醒模式"
PatternMatch = "Pattern Match喚醒模式"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Link Change喚醒模式"
SpeedDuplex = "速度和雙工"
FlowCtrl = "流量控制"
WakeFromShut = "從關閉狀態下喚醒"
BatSpeed = "電池狀態傳輸速度"
SmartSpeed = "智慧降速節能"
MaxSpeed = "全速"
BatLinkDet = "電池狀態鏈接偵測"
NoPwrSave = "無節能"
MaxPwrSave = "最大節能"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


; Chinese (PRC)
[Strings.0804]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "特大包"
ReceiveBuffers = "接收缓冲"
TransmitBuffers = "传送缓冲"
IPChksumOffv4 = "卸载 IPv4 检查和"
TCPChksumOffv4 = "卸载 TCP 检查和 (IPv4)"
TCPChksumOffv6 = "卸载 TCP 检查和 (IPv6)"
UDPChksumOffv4 = "卸载 UDP 检查和 (IPv4)"
UDPChksumOffv6 = "卸载 UDP 检查和 (IPv6)"
LSOv1 = "卸载超大发送 (IPv4)"
LSOv2IP4 = "卸载超大发送 v2 (IPv4)"
LSOv2IP6 = "卸载超大发送 v2 (IPv6)"
PriorityVLAN = "802.1p 优先级和 VLAN"
RSS = "受端负载调节"
TXEna = "启用 Tx"
RXEna = "启用 Rx"
TXRXEna = "启用Tx 和 Rx"
PrioVlanDis = "禁用优先级和 VLAN"
PrioEna = "启用优先级"
VlanEna = "启用VLAN"
PrioVlanEna = "启用优先级和 VLAN"
NetAddress   = "网络地址"
WakeUpCaps   = "唤醒功能"
IntMod = "中断模式"
MaxIrq = "最大 IRQ数量"
LogMsg = "日志状态信息"
RLMT  = "RLMT 模式"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "首选端口"
On = "开"
Off = "关"
Enabled = "启用"
Disabled = "禁用"
Non = "无"
Err = "错误"
Wrn = "警告"
Sta = "状态信息"
All = "所有信息"
A = "A"
B = "B"
Autosense = "自动感应"
10MHD = "10Mbps 半双工"
10MFD = "10Mbps 全双工"
100MHD = "100Mbps 半双工"
100MFD = "100Mbps 全双工"
MagicPacket = "Magic Packet唤醒模式"
PatternMatch = "Pattern Match唤醒模式"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Link Change唤醒模式"
SpeedDuplex = "速度和双工"
FlowCtrl = "流控制"
WakeFromShut = "从关闭状态下唤醒"
BatSpeed = "电池状态传输速度"
SmartSpeed = "智慧降速节能"
MaxSpeed = "全速"
BatLinkDet = "电池状态链接侦测"
NoPwrSave = "无节能"
MaxPwrSave = "最大节能"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


; German (Standard)
[Strings.0407]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Jumbo-Paket"
ReceiveBuffers = "Empfangspuffer"
TransmitBuffers = "Übertragungspuffer"
IPChksumOffv4 = "Verlagerung IPv4-Prüfsumme"
TCPChksumOffv4 = "Verlagerung TCP-Prüfsumme (IPv4)"
TCPChksumOffv6 = "Verlagerung TCP-Prüfsumme (IPv6)"
UDPChksumOffv4 = "Verlagerung UDP-Prüfsumme (IPv4)"
UDPChksumOffv6 = "Verlagerung UDP-Prüfsumme (IPv6)"
LSOv1 = "Übernahme TCP-Segment. (IPv4)"
LSOv2IP4 = "Übernahme TCP-Segment. V2 (IPv4)"
LSOv2IP6 = "Übernahme TCP-Segment. V2 (IPv6)"
PriorityVLAN = "802.1p Priorität & VLAN"
RSS = "Receive Side Scaling"
TXEna = "Tx aktiviert"
RXEna = "Rx aktiviert"
TXRXEna = "Tx & Rx aktiviert"
PrioVlanDis = "Priorität & VLAN deaktiviert"
PrioEna = "Priorität aktiviert"
VlanEna = "VLAN aktiviert"
PrioVlanEna = "Priorität & VLAN aktiviert"
NetAddress   = "Netzwerkadresse"
WakeUpCaps   = "Wake-up-Funktionen"
IntMod = "Interrupt-Moderation"
MaxIrq = "Max. IRQ pro Sek."
LogMsg = "Statusmeldungen protokollieren"
RLMT  = "RLMT-Modus"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Bevorzugter Port"
On = "Ein"
Off = "Aus"
Enabled = "Aktiviert"
Disabled = "Deaktiviert"
Non = "Keine"
Err = "Fehler"
Wrn = "Warnungen"
Sta = "Statusmeldungen"
All = "Alle Meldungen"
A = "A"
B = "B"
Autosense = "Automatische Erkennung"
10MHD = "10 Mbit/s Halbduplex"
10MFD = "10 Mbit/s Vollduplex"
100MHD = "100 Mbit/s Halbduplex"
100MFD = "100 Mbit/s Vollduplex"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Änderung des Linkstatus"
SpeedDuplex = "Geschwindigkeit und Duplexmodus"
FlowCtrl = "Datenflusskontrolle"
WakeFromShut = "Wake-up aus abgeschaltetem Zust."
BatSpeed = "Batteriemodus-Geschwindigkeit"
SmartSpeed = "Energiespar-Geschwindigkeit"
MaxSpeed = "Höchstgeschwindigkeit"
BatLinkDet = "Linkerkennung im Batteriemodus"
NoPwrSave = "Keine Energieeinsparung"
MaxPwrSave = "Maximale Energieeinsparung"
EnDetPwrSave = "EnergyDetect+™"










;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


; Spanish (Spain, Traditional Sort)
[Strings.040A]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Paquete Jumbo"
ReceiveBuffers = "Recibir búferes"
TransmitBuffers = "Transmitir búferes"
IPChksumOffv4 = "Desc. suma comp.IPv4"
TCPChksumOffv4 = "Desc. suma comp. TCP (IPv4)"
TCPChksumOffv6 = "Desc. suma comp. TCP (IPv6)"
UDPChksumOffv4 = "Desc. suma comp. UDP (IPv4)"
UDPChksumOffv6 = "Desc. suma comp. UDP (IPv6)"
LSOv1 = "Desc. envío grande (IPv4)"
LSOv2IP4 = "Desc. envío grande v2 (IPv4)"
LSOv2IP6 = "Desc. envío grande v2 (IPv6)"
PriorityVLAN = "802.1p prioridad y VLAN"
RSS = "Escala del lado de la recep."
TXEna = "Tx activado"
RXEna = "Rx activado"
TXRXEna = "Tx y Rx activados"
PrioVlanDis = "Prioridad y VLAN desactivados"
PrioEna = "Prioridad activada"
VlanEna = "VLAN activado"
PrioVlanEna = "Prioridad y VLAN activados"
NetAddress   = "Dirección de red"
WakeUpCaps   = "Capacidades de reactivación"
IntMod = "Moderación de interrupción"
MaxIrq = "IRQ máx. por seg."
LogMsg = "Mensajes de estado del registro"
RLMT  = "Modo RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Puerto preferido"
On = "Encendido"
Off = "Apagado"
Enabled = "Activado"
Disabled = "Desactivado"
Non = "Ninguna"
Err = "Errores"
Wrn = "Advertencias"
Sta = "Mensajes de estado"
All = "Todos los mensajes"
A = "A"
B = "B"
Autosense = "Orientación automática"
10MHD = "Dúplex media 10Mbps"
10MFD = "Dúplex completa 10Mbps"
100MHD = "Dúplex media 100Mbps"
100MFD = "Dúplex completa 100Mbps"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Cambio de enlace"
SpeedDuplex = "Velocidad y dúplex del enlace"
FlowCtrl = "Control de flujo"
WakeFromShut = "Wake From Shutdown"
BatSpeed = "BatterySpeedSettings"
SmartSpeed = "SmartSpeedDown"
MaxSpeed = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


; French (Standard)
[Strings.040C]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Paquet géant"
ReceiveBuffers = "Tampons de réception"
TransmitBuffers = "Tampons de transmission"
IPChksumOffv4 = "DéchargTotal de contrôle IPv4"
TCPChksumOffv4 = "DéchargTotalContrôle TCP(IPv4)"
TCPChksumOffv6 = "DéchargTotalContrôle TCP(IPv6)"
UDPChksumOffv4 = "DéchargTotalContrôle UDP(IPv4)"
UDPChksumOffv6 = "DéchargTotalContrôle UDP(IPv6)"
LSOv1 = "DéchargeEnvoiImportant (IPv4)"
LSOv2IP4 = "DéchargeEnvoiImportant v2 IPv4"
LSOv2IP6 = "DéchargeEnvoiImportant v2 IPv6"
PriorityVLAN = "Priorité 802.1p & VLAN"
RSS = "Distribution côté Rx"
TXEna = "Tx activée"
RXEna = "Rx activée"
TXRXEna = "Tx & Rx activées"
PrioVlanDis = "Priorité & VLAN désactivés"
PrioEna = "Priorité activée"
VlanEna = "VLAN activé"
PrioVlanEna = "Priorité & VLAN activés"

NetAddress   = "Adresse réseau"
WakeUpCaps   = "Capacités de réveil"
IntMod = "Modération de l'interruption"
MaxIrq = "IRQ max. par seconde"
LogMsg = "Messages d'état du journal"
RLMT  = "Mode RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Port préféré"
On = "Actif"
Off = "Inactif"
Enabled = "Activé(e)"
Disabled = "Désactivé(e)"
Non = "Aucun"
Err = "Erreurs"
Wrn = "Avertissements"
Sta = "Messages d'état"
All = "Tous les messages"
A = "A"
B = "B"
Autosense = "Détection automatique"
10MHD = "10 Mbits/s Semi-duplex"
10MFD = "10 Mbits/s Duplex intégral"
100MHD = "100 Mbits/s Semi-duplex"
100MFD = "100 Mbits/s Duplex intégral"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Changement du lien"
SpeedDuplex = "Vitesse de liaison et duplex"
FlowCtrl = "Contrôle de flux"
WakeFromShut = "Reveil de l'état arreté"
BatSpeed = "Vitesse en mode batterie"
SmartSpeed = "Reduction d'énergie"
MaxSpeed = "Pleine vitesse"
BatLinkDet = "Détection en mode batterie"
NoPwrSave = "Pas des économies d'énergie"
MaxPwrSave = "Économies d'énergie maximales"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


; Italian (Standard)
[Strings.0410]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Pacchetto jumbo"
ReceiveBuffers = "Buffer di ricezione"
TransmitBuffers = "Buffer di trasmissione"
IPChksumOffv4 = "Checksum Offload IPv4"
TCPChksumOffv4 = "Checksum Offload TCP (IPv4)"
TCPChksumOffv6 = "Checksum Offload TCP (IPv6)"
UDPChksumOffv4 = "Checksum Offload UDP (IPv4)"
UDPChksumOffv6 = "Checksum Offload UDP (IPv6)"
LSOv1 = "Large Send Offload (IPv4)"
LSOv2IP4 = "Large Send Offload v2 (IPv4)"
LSOv2IP6 = "Large Send Offload v2 (IPv6)"
PriorityVLAN = "Priorità & VLAN 802.1p"
RSS = "Receive Side Scaling"
TXEna = "Tx abilitato"
RXEna = "Rx abilitato"
TXRXEna = "Tx & Rx abilitati"
PrioVlanDis = "Priorità & VLAN disabil."
PrioEna = "Priorità abilitata"
VlanEna = "VLAN abilitato"
PrioVlanEna = "Priorità & VLAN abilitati"
NetAddress   = "Indirizzo di rete"
WakeUpCaps   = "Funzioni Wake Up "
IntMod = "Moderazione interrupt"
MaxIrq = "Max IRQ per sec"
LogMsg = "Messaggi di stato registro"
RLMT  = "Modalità RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Porta preferita"
On = "Attivato"
Off = "Disattivato"
Enabled = "Attivato"
Disabled = "Disattivato"
Non = "Nessuno"
Err = "Errori"
Wrn = "Avvertenze"
Sta = "Messaggi di stato"
All = "Tutti i messaggi"
A = "A"
B = "B"
Autosense = "Autoriconoscimento"
10MHD = "10Mbps half duplex"
10MFD = "10Mbps full duplex"
100MHD = "100Mbps half duplex"
100MFD = "100Mbps full duplex"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Cambio collegamento"
SpeedDuplex = "Velocità di collegamento e duplex"
FlowCtrl = "Controllo del flusso"
WakeFromShut = "Wake From Shutdown"
BatSpeed = "BatterySpeedSettings"
SmartSpeed = "SmartSpeedDown"
MaxSpeed = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


; Japanese
[Strings.0411]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "ジャンボ パケット"
ReceiveBuffers = "受信バッファ"
TransmitBuffers = "送信バッファ"
IPChksumOffv4 = "IPv4チェックサム オフロード"
TCPChksumOffv4 = "TCPチェックサム オフロード(IPv4)"
TCPChksumOffv6 = "TCPチェックサム オフロード(IPv6)"
UDPChksumOffv4 = "UDPチェックサム オフロード(IPv4)"
UDPChksumOffv6 = "UDPチェックサム オフロード(IPv6)"
LSOv1 = "大量送信オフロード (IPv4)"
LSOv2IP4 = "大量送信オフロード v2 (IPv4)"
LSOv2IP6 = "大量送信オフロード v2 (IPv6)"
PriorityVLAN = "802.1p 優先度オン & VLAN"
RSS = "RSS"
TXEna = "Tx 有効化"
RXEna = "Rx 有効化"
TXRXEna = "Tx & Rx 有効化"
PrioVlanDis = "優先度 & VLAN 無効化"
PrioEna = "優先度有効化"
VlanEna = "VLAN 有効化"
PrioVlanEna = "優先度 & VLAN 有効化"
NetAddress   = "ネットワークアドレス"
WakeUpCaps   = "ウェイク アップ機能"
IntMod = "割り込み節度"
MaxIrq = "毎秒最大 IRQ"
LogMsg = "ログ ステータス メッセージ"
RLMT  = "RLMTモード"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "優先ポート"
On = "オン"
Off = "オフ"
Enabled = "オン"
Disabled = "オフ"
Non = "なし"
Err = "エラー"
Wrn = "警告"
Sta = "ステータス メッセージ"
All = "全てのメッセージ"
A = "A"
B = "B"
Autosense = "自動感知"
10MHD = "10Mbps 半二重"
10MFD = "10Mbps 全二重"
100MHD = "100Mbps 半二重"
100MFD = "100Mbps 全二重"
MagicPacket = "マジック パケット"
PatternMatch = "パターン マッチ"
MagPackPattMatch = "マジック パケットとパターン マッチ"
LinkChange = "リンクの変更"
SpeedDuplex = "リンク速度とデュプレックス"
FlowCtrl = "フロー制御"
WakeFromShut = "シャットダウンからのウェイクアップ"
BatSpeed = "バッテリ速度設定"
SmartSpeed = "スマート速度制御"
MaxSpeed = "最大速度"
BatLinkDet = "バッテリ モード リンク検出"
NoPwrSave = "省エネなし"
MaxPwrSave = "最大省エネ"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


; Korean
[Strings.0412]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "점보 패킷"
ReceiveBuffers = "수신 버퍼"
TransmitBuffers = "송신 버퍼"
IPChksumOffv4 = "IPv4 검사합계 오프로드"
TCPChksumOffv4 = "TCP검사합계오프로드(IPv4)"
TCPChksumOffv6 = "TCP검사합계오프로드(IPv6)"
UDPChksumOffv4 = "UDP검사합계오프로드(IPv4)"
UDPChksumOffv6 = "UDP검사합계오프로드(IPv6)"
LSOv1 = "대량송신 오프로드(IPv4)"
LSOv2IP4 = "대량송신오프로드v2(IPv4)"
LSOv2IP6 = "대량송신오프로드v2(IPv6)"
PriorityVLAN = "802.1p우선순위&VLAN"
RSS = "수신 성능 확장 구조"
TXEna = "Tx 사용"
RXEna = "Rx 사용"
TXRXEna = "Tx & Rx 사용"
PrioVlanDis = "우선순위&VLAN미사용"
PrioEna = "우선순위 사용"
VlanEna = "VLAN 사용"
PrioVlanEna = "우선순위&VLAN 사용"
NetAddress   = "네트워크 주소"
WakeUpCaps   = "시스템 켜기 기능"
IntMod = "인터럽트 완화"
MaxIrq = "초당 최대 IRQ"
LogMsg = "로그 상태 메시지"
RLMT  = "RLMT 모드"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "기본 설정 포트"
On = "켜기"
Off = "끄기"
Enabled = "활성화됨"
Disabled = "활성 해제됨"
Non = "없음"
Err = "오류"
Wrn = "경고"
Sta = "상태 메시지"
All = "모든 메시지"
A = "A"
B = "B"
Autosense = "자동 감지"
10MHD = "10Mbps 반이중"
10MFD = "10Mbps 전이중"
100MHD = "100Mbps 반이중"
100MFD = "100Mbps 전이중"
MagicPacket = "매직 패킷"
PatternMatch = "패턴 일치"
MagPackPattMatch = "매직 패킷 및 패턴 일치"
LinkChange = "링크 변경"
SpeedDuplex = "링크 속도 및 이중성"
FlowCtrl = "흐름 제어"
WakeFromShut = "종료 상태에서 깨우기"
BatSpeed = "배터리속도설정"
SmartSpeed = "스마트감속"
MaxSpeed = "최대속도"
BatLinkDet = "배터리모델링크감지"
NoPwrSave = "절전안함"
MaxPwrSave = "최대절전"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


; Polish
[Strings.0415]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Pakiet Jumbo"
ReceiveBuffers = "Bufory odbioru"
TransmitBuffers = "Bufory nadawcze"
IPChksumOffv4 = "IPv4 ob. sumy kon."
TCPChksumOffv4 = "ob. sumy kon. pak. TCP (IPv4)"
TCPChksumOffv6 = "ob. sumy kon. pak. TCP (IPv6)"
UDPChksumOffv4 = "ob. sumy kon. pak. UDP (IPv4)"
UDPChksumOffv6 = "ob. sumy kon. pak. UDP (IPv6)"
LSOv1 = "obs. wys. du. il da.(IPv4)"
LSOv2IP4 = "obs. wys. du. il da. v2 (IPv4)"
LSOv2IP6 = "obs. wys. du. il da. v2 (IPv6)"
PriorityVLAN = "802.1p Priorytet & VLAN"
RSS = "roz. ru. przy. do wiel. ukł."
TXEna = "Bufory nadawcze wł."
RXEna = "Bufory odbiorcze wł."
TXRXEna = "Buf. nad. & odb. wł."
PrioVlanDis = "Priorytet & VLAN wył."
PrioEna = "Priorytet wł."
VlanEna = "VLAN Włączony"
PrioVlanEna = "Priorytet & VLAN wł."
NetAddress   = "Adres sieciowy"
WakeUpCaps   = "Funkcje budzenia"
IntMod = "Moderacja przerwania"
MaxIrq = "Maks. IRQ na sek."
LogMsg = "Zapisywanie komunikatów o stat."
RLMT  = "RLMT Mode"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Preferowany port"
On = "Włączone"
Off = "Wyłączone"
Enabled = "Włączony"
Disabled = "Wyłączony"
Non = "Żadne"
Err = "Błędy"
Wrn = "Ostrzeżenia"
Sta = "Komunikaty o stanie"
All = "Wszystkie komunikaty"
A = "A"
B = "B"
Autosense = "Automatyczne wykrywanie"
10MHD = "10 Mbps Półdupleks"
10MFD = "10 Mbps Pełen dupleks"
100MHD = "100 Mbps Półdupleks"
100MFD = "100 Mbps Pełen dupleks"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Zmiana łącza"
SpeedDuplex = "Szybkość i Dupleks"
FlowCtrl = "Kontrola przepływu danych"
WakeFromShut = "Uaktywnianie z Wyłączenia"
BatSpeed = "Szybkość w trybie bateryjnym"
SmartSpeed = "Zmniejszona szybkość łącza"
MaxSpeed = "Maksymalna szybkość łącza"
BatLinkDet = "Wykrywanie łącza w trybie bat."
NoPwrSave = "Bez oszczędności energii"
MaxPwrSave = "Maks. oszczędność energii"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


; Portuguese (Brazil)
[Strings.0416]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Pacote Jumbo"
ReceiveBuffers = "Buffers de Recepção"
TransmitBuffers = "Buffers de Transmissão"
IPChksumOffv4 = "Descarga Soma de Verif. IPv4"
TCPChksumOffv4 = "Desc. Soma Verif. TCP (IPv4)"
TCPChksumOffv6 = "Desc. Soma Verif. TCP (IPv6)"
UDPChksumOffv4 = "Desc. Soma Verif. UDP (IPv4)"
UDPChksumOffv6 = "Desc. Soma Verif. UDP (IPv6)"
LSOv1 = "Grande Desc. Envio (IPv4)"
LSOv2IP4 = "Grande Desc. Envio v2 (IPv4)"
LSOv2IP6 = "Grande Desc. Envio v2 (IPv6)"
PriorityVLAN = "802.1p Prior. & VLAN"
RSS = "Escalamento Lado Receptor"
TXEna = "Tx habilitado"
RXEna = "Rx habilitado"
TXRXEna = "Tx & Rx habilitado"
PrioVlanDis = "Prior. & VLAN desabil."
PrioEna = "Prioridade habilitada"
VlanEna = "VLAN habilitado"
PrioVlanEna = "Prioridade & VLAN habil."

NetAddress   = "Endereço de Rede"
WakeUpCaps   = "Capacidades de Despertar"
IntMod = "Moderação de Interrupção"
MaxIrq = "IRQ Máx por Seg"
LogMsg = "Registrar Mensagens de Estado"
RLMT  = "Modo RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Porta Preferida"
On = "Ligado"
Off = "Desligado"
Enabled = "Ativado"
Disabled = "Desativado"
Non = "Nenhum"
Err = "Erros"
Wrn = "Avisos"
Sta = "Mensagens de Estado"
All = "Todas as Mensagens"
A = "A"
B = "B"
Autosense = "Autodetecção"
10MHD = "Semi Dúplex 10Mbps"
10MFD = "Dúplex Completo 10Mbps"
100MHD = "Semi Dúplex 100Mbps"
100MFD = "Dúplex Completo100Mbps"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Troca de Vínculo"
SpeedDuplex = "Velocidade de link e duplex"
FlowCtrl = "Controle de Fluxo"
WakeFromShut = "Wake From Shutdown"
BatSpeed = "BatterySpeedSettings"
SmartSpeed = "SmartSpeedDown"
MaxSpeed = "FullSpeed"
BatLinkDet = "BatteryModeLinkDetection"
NoPwrSave = "NoEnergySaving"
MaxPwrSave = "MaximumEnergySaving"
EnDetPwrSave = "EnergyDetect+™"
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"


; Russian
[Strings.0419]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
D-Link = "D-Link"
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
JumboPacket = "Большой пакет"
ReceiveBuffers = "Буферы приема"
TransmitBuffers = "Буферы передачи"
IPChksumOffv4 = "Разг.контр.суммы IPv4"
TCPChksumOffv4 = "Разг.контр.суммы TCP (IPv4)"
TCPChksumOffv6 = "Разг.контр.суммы TCP (IPv6)"
UDPChksumOffv4 = "Разг.контр.суммы UDP (IPv4)"
UDPChksumOffv6 = "Разг.контр.суммы UDP (IPv6)"
LSOv1 = "Разг.больш.передач (IPv4)"
LSOv2IP4 = "Разг.больш.передач v2 (IPv4)"
LSOv2IP6 = "Разг.больш.передач v2 (IPv6)"
PriorityVLAN = "802.1p приоритет и VLAN"
RSS = "Масшт. на стор. приемника"
TXEna = "Tx включен"
RXEna = "Rx включен"
TXRXEna = "Tx & Rx включен"
PrioVlanDis = "Приоритет и VLAN откл."
PrioEna = "Приоритет включен"
VlanEna = "VLAN включен"
PrioVlanEna = "Приоритет и VLAN вкл."
NetAddress   = "Сетевой адрес"
WakeUpCaps   = "Возможности пробуждения"
IntMod = "Управление прерываниями"
MaxIrq = "Макс. IRQ - шт/сек."
LogMsg = "Записывать статус. сообщения"
RLMT  = "Режим RLMT"
Link  = "CLS"   
OtherPort    = "CLP" 
Segment = "CLPSS" 
Preferred    = "Предпочтительный порт"
On = "Вкл."
Off = "Выкл."
Enabled = "Включать" 
Disabled = "Отключать"
Non = "Нет"
Err = "Ошибки"
Wrn = "Предупреждения"
Sta = "Статусные сообщения"
All = "Все сообщения"
A = "A"
B = "B"
Autosense = "Автоопределение"
10MHD = "10Мбит/с полудуплекс"
10MFD = "10Мбит/с полный дуплекс"
100MHD = "100Мбит/с полудуплекс"
100MFD = "100Мбит/с полный дуплекс"
MagicPacket = "Magic Packet"
PatternMatch = "Pattern Match"
MagPackPattMatch = "Magic Packet & Pattern Match"
LinkChange = "Измен. статуса соединения"
SpeedDuplex = "Скорость и дуплекс"
FlowCtrl = "Управление потоком данных"
WakeFromShut = "Просыпаться от выключение"
BatSpeed = "Cкорость передачи от батареи"
SmartSpeed = "Уменьшение скорости"
MaxSpeed = "Макс. скорость передачи"
BatLinkDet = "Обнаружение канала от батареи"
NoPwrSave = "Без экономии энергии"
MaxPwrSave = "Mакс. экономии энергии"
EnDetPwrSave = "EnergyDetect+™"

;; Do NOT translate
;---------------------------------------------------------------------------------------------------
DriverDisk = "D-Link Gigabit Ethernet Adapter Installation Disk"


Yukon-4001.DeviceDesc = "D-Link DGE-550SX PCI-X Gigabit Ethernet Adapter"
Yukon-4346.DeviceDesc = "D-Link DGE-560SX Single Fiber Gigabit Ethernet PCI-E Adapter V.A1"
Yukon-4B00.DeviceDesc = "D-Link DGE-560T PCI Express Gigabit Ethernet Adapter"
Yukon-4B01.DeviceDesc = "D-Link DGE-530T V.B1 Gigabit Ethernet Adapter"
Yukon-4B02.DeviceDesc = "D-Link DGE-560SX PCI Express Gigabit Ethernet Adapter"
Yukon-4C00.DeviceDesc = "D-Link DGE-530T Gigabit Ethernet Adapter"
m4cxvst64.DriverDesc	= "NDIS6.0 Miniport Driver for D-Link Gigabit Ethernet Controller"
