; EN2228.INF for Win 98 & Win 2000
;
; 10/100 Base FastEthernet PC Card
;

[Version]
signature  = "$Windows NT$"
Class=Net
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%V_PCCARD%
LayoutFile=layout.inf, layout1.inf

[Manufacturer]
%V_PCCARD%=PCCARD

[PCCARD]
%*EN2228.DeviceDesc%=EN2228.ndi,PCMCIA\CHEETAH_ETHERCARD-EN2228-71C2

[EN2228.ndi.NT]
Characteristics = 0x4
BusType         = 8
AddReg          = EN2228cc.ndi.reg, common.reg
CopyFiles = EN2228.ndis5.CopyFiles

[EN2228.ndi.NT.Services]
AddService = EN2228, 2, EN2228.Service, EN2228.AddEventLog

[Common.reg]
HKR,Ndi\params\ConnectionType,ParamDesc,,"Connection Type"
HKR,Ndi\params\ConnectionType,default,,0
HKR,Ndi\params\ConnectionType,type,,enum
HKR,Ndi\params\ConnectionType\enum,0,,"AutoSense"
HKR,Ndi\params\ConnectionType\enum,8,,"100BaseTx"
HKR,Ndi\params\ConnectionType\enum,2,,"10BaseT (Twisted_Pair)"



[EN2228cc.ndi.reg]
HKR, Ndi,               Service,    0, "EN2228"
HKR, Ndi\Interfaces,    LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces,    UpperRange, 0, "ndis5"
HKR,               ,    Pcmcia    , 0, "2"

[EN2228.ndis5.CopyFiles]
EN2228.sys,,,2

[EN2228.Service]
DisplayName     =   %Service.DispName%
ServiceType     =   1 ;%SERVICE_KERNEL_DRIVER%
StartType       =   3 ;%SERVICE_AUTO_START%
ErrorControl    =   1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   =   %12%\EN2228.sys
LoadOrderGroup  =   NDIS
AddReg          =   TextModeFlags.reg

[EN2228.AddEventLog]
AddReg = EN2228.AddEventLog.reg

[EN2228.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000,"%%SystemRoot%%\System32\netevent.dll"
HKR,    ,   TypesSupported,     0x00010001, 7

[TextModeFlags.reg]
HKR, , TextModeFlags, 0x00010001, 0x0001

;---------------

[EN2228.ndi]
AddReg=EN2228.ndi.reg,EN2228.params.reg
LogConfig=EN2228.LogConfigOverride
CopyFiles=EN2228.ndis3.CopyFiles
CopyFiles=Inf.CopyFiles

[EN2228.LogConfigOverride]
IRQConfig=3,4,5,7,9,10,11,12,13,15
IOConfig=20@200-3FF%FFE0(3FF::)
ConfigPriority = NORMAL

[EN2228.ndi.reg]
HKR,,DevLoader,0,*ndis
HKR,,DeviceVxDs,0,EN2228.sys
HKR,,EnumPropPages,0,netdi.dll
HKR,Ndi,DeviceID,0,PCMCIA\CHEETAH_ETHERCARD-EN2228-71C2
HKR,Ndi,CardType,0,PCMCIA
HKR,NDIS,LogDriverName,0,EN2228
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0a
HKR,Ndi\Interfaces,DefUpper,0,ndis3
HKR,Ndi\Interfaces,DefLower,0,ethernet
HKR,Ndi\Interfaces,UpperRange,0,ndis3
HKR,Ndi\Interfaces,LowerRange,0,ethernet
; Install sectioins
HKR,Ndi\Install,ndis3,,"EN2228.ndis3"

[EN2228.params.reg]
HKR,,InterruptNumber,1,04,00,00,00
HKR,Ndi\params\InterruptNumber,resc,1,04,00,00,00
HKR,Ndi\params\interruptNumber,ParamDesc,,"Interrupt Level"
HKR,Ndi\params\InterruptNumber,flag,1,60,00,00,00

HKR,,IOBaseAddress,1,02,00,00,00
HKR,Ndi\params\IOBaseAddress,resc,1,02,00,00,00
HKR,Ndi\params\IOBaseAddress,ParamDesc,,"I/O Base Address"
HKR,Ndi\params\IOBaseAddress,flag,1,20,00,00,00

HKR,Ndi\params\ConnectionType,ParamDesc,,"Connection Type"
HKR,Ndi\params\ConnectionType,default,,0
HKR,Ndi\params\ConnectionType,type,,enum
HKR,Ndi\params\ConnectionType\enum,0,,"AutoSense"
HKR,Ndi\params\ConnectionType\enum,8,,"100BaseTx"
HKR,Ndi\params\ConnectionType\enum,2,,"10BaseT (Twisted_Pair)"

[EN2228.ndis3]
CopyFiles=EN2228.ndis3.CopyFiles

[EN2228.ndis3.CopyFiles]
EN2228.SYS

[Inf.CopyFiles]
EN2228.INF

[SourceDisksNames]
1="CHEETAH ETHERCARD EN2228 Installation Diskette", "",

[SourceDisksFiles]
EN2228.SYS=1
EN2228.INF=1

[DestinationDirs]
DefaultDestDir=11
EN2228.ndis3.CopyFiles       =11
Inf.CopyFiles =17 ; Windows 95 Inf Directory
EN2228.ndis5.CopyFiles  =   12

;****************************************************************************
; Localizable Strings
;****************************************************************************
[strings]
Service.DispName =   "CHEETAH ETHERCARD EN2228 NT Driver"
; Provider
; Manufacturers
V_PCCARD="CHEETAH"
; PNP Devices
*EN2228.DeviceDesc="CHEETAH ETHERCARD EN2228"
