;===========================================================================
; 
; Vista NDIS driver INF for Libertas 802.11 Wireless
; Copyright (C) 2005-2006 Marvell Semiconductor, Inc.
;
;=========================================================================== 

[Version] 
Signature = "$Windows NT$" 
Compatible  = 1
Class=Net
ClassGUID={4D36E972-E325-11CE-BFC1-08002BE10318} 
Provider=%MRVL% 
CatalogFile=MRVW24B.cat
DriverVer=03/19/2008, 1.0.5.2

;===========================================================================
; Source Media Information Sections
;===========================================================================
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
; On Marvell installation disk 1 
MRVW24B.sys = 1

[DestinationDirs]
W8360USB.x32.CopyFiles  = 12 

DefaultDestDirs    = 11

[Manufacturer] 
%MRVL%=Marvell,NTx86.6.0

[Marvell.NTx86.6.0]
%MRVL8360USB.DeviceDesc% = W8360USBx32.ndi,USB\VID_1286&PID_2006
%BelkinN1USB.DeviceDesc% = W8360USBx32.ndi,USB\VID_1799&PID_8051
%LinksysNUSB.DeviceDesc% = W8360USBx32.ndi,USB\VID_13B1&PID_0029
%WN121TUSB.DeviceDesc%   = W8360USBx32.ndi,USB\VID_0846&PID_7100
%WN111USB.DeviceDesc%    = W8360USBx32.ndi,USB\VID_0846&PID_9000
%N650USB.DeviceDesc%     = W8360USBx32.ndi,USB\VID_07D1&PID_3B10
%AsusUSB1.DeviceDesc%    = W8360USBx32.ndi,USB\VID_0B05&PID_172A
%AsusUSB2.DeviceDesc%    = W8360USBx32.ndi,USB\VID_0B05&PID_172B
%BuffaloUSB1.DeviceDesc%  = W8360USBx32.ndi,USB\VID_0411&PID_00CA
%BuffaloUSB2.DeviceDesc%  = W8360USBx32.ndi,USB\VID_0411&PID_00CB
%DLinkUSB.DeviceDesc%	 = W8360USBx32.ndi,USB\VID_07D1&PID_3B11
;===========================================================================
; ControlFlags section
;===========================================================================
[ControlFlags]
ExcludeFromSelect = *

;***************************************************************************
;**         
;**          Windows DDInstall section
;**          
;***************************************************************************
;***************************************************************************
[W8360USBx32.ndi]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI ,CardBus or USB
BusType         = 15 ;Is USB
AddReg          = W8360USB.reg, W8360USBx32.reg
CopyFiles       = W8360USB.x32.CopyFiles
*IfType 	= 71 ; If_TYPE_IEEE80211
*MediaType      = 16    ; NdisMediumNative802_11
*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11

[W8360USBx32.ndi.Services]
AddService = MRV6X32U, 2, W8360USBx32.Service, CommonXP.EventLog

;===========================================================================
; W8335a PCI WinXP registers
;===========================================================================
[W8360USBx32.reg]
HKR, Ndi,            Service,    0, "MRVW24B"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5,mrvl_prot"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet,wlan"


[W8360USB.x32.CopyFiles]
MRVW24B.sys,,,2 

[W8360USBx32.Service]
DisplayName    = %W8360USBx32.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\MRVW24B.sys
LoadOrderGroup = NDIS


[CommonXP.EventLog]
AddReg = CommonXP.AddEventLog.reg

[CommonXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;===========================================================================
; W8335a PCI common, MIB can be defined here
;===========================================================================
[W8360USB.reg]
;
; LED Control
;
; Mode 1 (Default)
HKR,, LED0PowerOn,		0x00002, "0100ff00"
HKR,, LED1PowerOn,		0x00002, "0101fe00"
HKR,, LED0PowerOff,		0x00002, "0100fe00"
HKR,, LED1PowerOff,		0x00002, "0101fe00"
HKR,, LED0Scan,			0x00002, "0100ff00"
HKR,, LED1Scan,			0x00002, "01010200"
HKR,, LED0Associated,		0x00002, "0100ff00"
HKR,, LED1Associated,		0x00002, "0101fe00"
HKR,, LED0Joined,		0x00002, "0100ff00"
HKR,, LED1Joined,		0x00002, "0101fe00"
HKR,, LED0Started,		0x00002, "0100ff00"
HKR,, LED1Started,		0x00002, "0101fe00"
HKR,, LED0Tx,			0x00002, "0100ff00"
HKR,, LED1Tx,			0x00002, "01010200"
HKR,, LED0Rx,			0x00002, "0100ff00"
HKR,, LED1Rx,			0x00002, "01010200"
;HKR,, LED0TxMiddle,		0x00002, "0100ff00"
;HKR,, LED1TxMiddle,		0x00002, "01010200"
;HKR,, LED0RxMiddle,		0x00002, "0100ff00"
;HKR,, LED1RxMiddle,		0x00002, "01010200"
HKR,, LED0TxHigh,		0x00002, "0100ff00"
HKR,, LED1TxHigh,		0x00002, "01010200"
HKR,, LED0RxHigh,		0x00002, "0100ff00"
HKR,, LED1RxHigh,		0x00002, "01010200"

HKR,, LEDOffAfterRadioOff,	0x00002, "1" 

HKR, Ndi\params\AdhocMode,ParamDesc,,"%AdhocMode%"
HKR, Ndi\params\AdhocMode,default,,"1"
HKR, Ndi\params\AdhocMode,type,,enum
HKR, Ndi\params\AdhocMode\enum,"0",,"%AdhocMode_GMode%"
HKR, Ndi\params\AdhocMode\enum,"1",,"%AdhocMode_BMode%" 
HKR, Ndi\params\AdhocMode\enum,"4",,"%AdhocMode_NMode%" 

HKR, Ndi\params\TxPowerLvl,ParamDesc,,"%TxPowerLvlStr%"
HKR, Ndi\params\TxPowerLvl,default,,"3"
HKR, Ndi\params\TxPowerLvl,type,,enum
HKR, Ndi\params\TxPowerLvl\enum,"1",,"%LowPower%"
HKR, Ndi\params\TxPowerLvl\enum,"2",,"%MediumPower%" 
HKR, Ndi\params\TxPowerLvl\enum,"3",,"%HighPower%"
HKR, Ndi\params\TxPowerLvl\enum,"4",,"%VeryLowPower%" 


HKR, Ndi\xparams\DesiredSSID,ParamDesc,,"%SSID%"
HKR, Ndi\xparams\DesiredSSID,default,,""
HKR, Ndi\xparams\DesiredSSID,type,,"edit" 
HKR, Ndi\xparams\DesiredSSID,LimitText,,"32"
HKR, Ndi\xparams\DesiredSSID,UpperCase,,"0" 
HKR, Ndi\xparams\DesiredSSID,Optional,,"1" 

HKR, Ndi\xparams\AuthMode,ParamDesc,,"%AuthMode%"
HKR, Ndi\xparams\AuthMode,default,,"0"
HKR, Ndi\xparams\AuthMode,type,,enum
HKR, Ndi\xparams\AuthMode\enum,"0",,"%Open%"
HKR, Ndi\xparams\AuthMode\enum,"1",,"%Shared%"

HKR, Ndi\xparams\NetworkMode,ParamDesc,,"%NetworkMode%"
HKR, Ndi\xparams\NetworkMode,default,,"1"
HKR, Ndi\xparams\NetworkMode,type,,enum
HKR, Ndi\xparams\NetworkMode\enum,"0",,"%AdHoc%"
HKR, Ndi\xparams\NetworkMode\enum,"1",,"%Infrastructure%"

;HKR, Ndi\xparams\Wireless,ParamDesc,,"%WirelessM%"
;HKR, Ndi\xparams\Wireless,default,,"0"
;HKR, Ndi\xparams\Wireless,type,,enum
;HKR, Ndi\xparams\Wireless\enum,"0",,"Auto"
;HKR, Ndi\xparams\Wireless\enum,"1",,"B rates only"
 
HKR, Ndi\params\FragThsd,  ParamDesc,0 , "%FragThsds%"
HKR, Ndi\params\FragThsd,  default, 0 , "2346"
HKR, Ndi\params\FragThsd,  min, 0 , "256"
HKR, Ndi\params\FragThsd,  max, 0 , "2346"
HKR, Ndi\params\FragThsd,  step, 0 , "1"
HKR, Ndi\params\FragThsd,  Base, 0 , "10"
HKR, Ndi\params\FragThsd,  type, 0 ,"dword"

HKR, Ndi\xparams\Channel,  ParamDesc,0 , "%Channel%"
HKR, Ndi\xparams\Channel,  default, 0 , "36"
HKR, Ndi\xparams\Channel,  min, 0 , "1"
HKR, Ndi\xparams\Channel,  max, 0 , "165"
HKR, Ndi\xparams\Channel,  step, 0 , "1"
HKR, Ndi\xparams\Channel,  Base, 0 , "10"
HKR, Ndi\xparams\Channel,  type, 0 ,"dword"

HKR, Ndi\xparams\TxAntenna,  ParamDesc,0 , "%TxAntennaStr%"
HKR, Ndi\xparams\TxAntenna,  default, 0 , "2"
HKR, Ndi\xparams\TxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\TxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\TxAntenna,  type, 0 ,"dword"

HKR, Ndi\xparams\RxAntenna,  ParamDesc,0 , "%RxAntennaStr%"
HKR, Ndi\xparams\RxAntenna,  default, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\RxAntenna,  type, 0 ,"dword"

HKR, Ndi\params\RTSThsd,  ParamDesc, 0, "%RTSThsds%"
HKR, Ndi\params\RTSThsd,  default, 0, "2347"
HKR, Ndi\params\RTSThsd,  min, 0, "0"
HKR, Ndi\params\RTSThsd,  max, 0, "2347"
HKR, Ndi\params\RTSThsd,  step, 0, "1"
HKR, Ndi\params\RTSThsd,  Base, 0, "10"
HKR, Ndi\params\RTSThsd,  type, 0, "dword"

;HKR, Ndi\params\PowerMode,ParamDesc,,"%PowerMode%"
;HKR, Ndi\params\PowerMode,default,,"0"
;HKR, Ndi\params\PowerMode,type,,enum
;HKR, Ndi\params\PowerMode\enum,"0",,"CAM-Constantly Awake Mode"
;HKR, Ndi\params\PowerMode\enum,"1",,"MaxPSP-Max Power Savings"
;HKR, Ndi\params\PowerMode\enum,"2",,"FastPSP-Fast Power Savings"

HKR, Ndi\xparams\DataRate,ParamDesc,,"%DataRate%"
HKR, Ndi\xparams\DataRate,default,,"FF"
HKR, Ndi\xparams\DataRate,type,,enum
HKR, Ndi\xparams\DataRate\enum,"FF",,"%Auto%"
HKR, Ndi\xparams\DataRate\enum,"2",,"%Rate1%"
HKR, Ndi\xparams\DataRate\enum,"4",,"%Rate2%"
HKR, Ndi\xparams\DataRate\enum,"b",,"%Rate5%"
HKR, Ndi\xparams\DataRate\enum,"16",,"%Rate11%"
;HKR, Ndi\xparams\DataRate\enum,"2C",,"%Rate22%" 
HKR, Ndi\xparams\DataRate\enum,"C",,"%Rate6%" 
HKR, Ndi\xparams\DataRate\enum,"12",,"%Rate9%" 
HKR, Ndi\xparams\DataRate\enum,"18",,"%Rate12%" 
HKR, Ndi\xparams\DataRate\enum,"24",,"%Rate18%" 
HKR, Ndi\xparams\DataRate\enum,"30",,"%Rate24%" 
HKR, Ndi\xparams\DataRate\enum,"48",,"%Rate36%" 
HKR, Ndi\xparams\DataRate\enum,"60",,"%Rate48%" 
HKR, Ndi\xparams\DataRate\enum,"6C",,"%Rate54%"

HKR, Ndi\xparams\WepStatus,ParamDesc,,"%WepStatus%"
HKR, Ndi\xparams\WepStatus,default,,"1"
HKR, Ndi\xparams\WepStatus,type,,enum
HKR, Ndi\xparams\WepStatus\enum,"0",,"%Enabled%"
HKR, Ndi\xparams\WepStatus\enum,"1",,"%Disabled%"

HKR, Ndi\params\Preamble,ParamDesc,,"%PreambleStr%"
HKR, Ndi\params\Preamble,default,,"3"
HKR, Ndi\params\Preamble,type,,enum 
HKR, Ndi\params\Preamble\enum,"1",,"%Auto%"
HKR, Ndi\params\Preamble\enum,"2",,"%ShortPreamble%" 
HKR, Ndi\params\Preamble\enum,"3",,"%LongPreamble%"

;HKR, Ndi\params\DefaultAdhocMediaMode,ParamDesc,,"%DefaultAdhocMediaModeStr%"
;HKR, Ndi\params\DefaultAdhocMediaMode,default,,"0"
;HKR, Ndi\params\DefaultAdhocMediaMode,type,,enum 
;HKR, Ndi\params\DefaultAdhocMediaMode\enum,"0",,"%Band11b%"
;HKR, Ndi\params\DefaultAdhocMediaMode\enum,"1",,"%Band11g%" 
;HKR, Ndi\params\DefaultAdhocMediaMode\enum,"2",,"%Band11a%"

HKR, Ndi\params\AdhocChannel,ParamDesc,,"%AdhocChannelStr%"
HKR, Ndi\params\AdhocChannel,default,,"0"
HKR, Ndi\params\AdhocChannel,type,,enum
HKR, Ndi\params\AdhocChannel\enum,"0",,"Auto"
HKR, Ndi\params\AdhocChannel\enum,"1",,"Channel  1"
HKR, Ndi\params\AdhocChannel\enum,"2",,"Channel  2"
HKR, Ndi\params\AdhocChannel\enum,"3",,"Channel  3"
HKR, Ndi\params\AdhocChannel\enum,"4",,"Channel  4"
HKR, Ndi\params\AdhocChannel\enum,"5",,"Channel  5" 
HKR, Ndi\params\AdhocChannel\enum,"6",,"Channel  6" 
HKR, Ndi\params\AdhocChannel\enum,"7",,"Channel  7" 
HKR, Ndi\params\AdhocChannel\enum,"8",,"Channel  8" 
HKR, Ndi\params\AdhocChannel\enum,"9",,"Channel  9" 
HKR, Ndi\params\AdhocChannel\enum,"10",,"Channel 10" 
HKR, Ndi\params\AdhocChannel\enum,"11",,"Channel 11" 

HKR,, TxWepKey, 2, "" 
HKR,, WepKey1, 2, "" 
HKR,, WepKey2, 2, "" 
HKR,, WepKey3, 2, "" 
HKR,, WepKey4, 2, "" 

;HKR,, IntlRoaming, 2, "0"
HKR, Ndi\params\IntlRoaming,ParamDesc,,"%IntlRoaming%"
HKR, Ndi\params\IntlRoaming,default,,"0"
HKR, Ndi\params\IntlRoaming,type,,enum 
HKR, Ndi\params\IntlRoaming\enum,"0",,"%Disabled%"
HKR, Ndi\params\IntlRoaming\enum,"1",,"%Enabled%" 

HKR,, AMSDUCompatible,2, "1"
HKR,, AMPDUCompatible,2, "1"
HKR,, WiFi_Mode,2, "0"

;HKR, Ndi\params\BlockAckMode,ParamDesc,,"%AMPDUSettings%"
;HKR, Ndi\params\BlockAckMode,default,,"2"
;HKR, Ndi\params\BlockAckMode,type,,enum 
;HKR, Ndi\params\BlockAckMode\enum,"2",,"%Partial%" 
;HKR, Ndi\params\BlockAckMode\enum,"3",,"%Full%"

HKR, Ndi\params\EncryptionType,ParamDesc,,"%EncryptionType%"
HKR, Ndi\params\EncryptionType,default,,"0"
HKR, Ndi\params\EncryptionType,type,,enum 
HKR, Ndi\params\EncryptionType\enum,"0",,"%HwEncryption%" 
HKR, Ndi\params\EncryptionType\enum,"1",,"%SwEncryption%"

HKR, Ndi\params\EWCTurboMode,ParamDesc,,"%EWCTurboMode%"
HKR, Ndi\params\EWCTurboMode,default,,"1"
HKR, Ndi\params\EWCTurboMode,type,,enum 
HKR, Ndi\params\EWCTurboMode\enum,"0",,"%Disabled%"
HKR, Ndi\params\EWCTurboMode\enum,"1",,"%Enabled%" 

HKR, Ndi\params\HTModeEnabled
HKR, Ndi\params\HTModeEnabled, ParamDesc,,"%HTModeEnabled%"
HKR, Ndi\params\HTModeEnabled, default,,"1"
HKR, Ndi\params\HTModeEnabled, type,,enum
HKR, Ndi\params\HTModeEnabled\enum,"0",,"%Disabled%" 
HKR, Ndi\params\HTModeEnabled\enum,"1",,"%Enabled%"

HKR, Ndi\params\ChannelWidth, ParamDesc,,"%ChannelWidth%"
HKR, Ndi\params\ChannelWidth, default,,"-1"
HKR, Ndi\params\ChannelWidth, type,,enum
HKR, Ndi\params\ChannelWidth\enum,"0",,"%20MHz%" 
HKR, Ndi\params\ChannelWidth\enum,"1",,"%40MHz%"
HKR, Ndi\params\ChannelWidth\enum,"-1",,"%Auto%"

HKR, Ndi\params\ExtChannelOffset, ParamDesc,,"%ExtChannelOffset%"
HKR, Ndi\params\ExtChannelOffset, default,,"-1"
HKR, Ndi\params\ExtChannelOffset, type,,enum
HKR, Ndi\params\ExtChannelOffset\enum,"0",,"%Below%" 
HKR, Ndi\params\ExtChannelOffset\enum,"1",,"%Above%"
HKR, Ndi\params\ExtChannelOffset\enum,"2",,"%None%"
HKR, Ndi\params\ExtChannelOffset\enum,"-1",,"%Auto%"

HKR, Ndi\params\GuardInterval, ParamDesc,,"%GuardInterval%"
HKR, Ndi\params\GuardInterval, default,,"-1"
HKR, Ndi\params\GuardInterval, type,,enum
HKR, Ndi\params\GuardInterval\enum,"0",,"%LongGI%" 
HKR, Ndi\params\GuardInterval\enum,"1",,"%ShortGI%"
HKR, Ndi\params\GuardInterval\enum,"-1",,"%Auto%"

HKR, Ndi\params\RegistryMimoCfg, ParamDesc,,"%Antenna%"
HKR, Ndi\params\RegistryMimoCfg, default,,"-1"
HKR, Ndi\params\RegistryMimoCfg, type,,enum
HKR, Ndi\params\RegistryMimoCfg\enum,"0",,"%2by3%" 
HKR, Ndi\params\RegistryMimoCfg\enum,"1",,"%Antenna_A%"
HKR, Ndi\params\RegistryMimoCfg\enum,"2",,"%Antenna_B%"
HKR, Ndi\params\RegistryMimoCfg\enum,"3",,"%2by2%"
HKR, Ndi\params\RegistryMimoCfg\enum,"4",,"%Aby2%"
HKR, Ndi\params\RegistryMimoCfg\enum,"5",,"%Bby2%"
HKR, Ndi\params\RegistryMimoCfg\enum,"-1",,"%Auto%"

;HKR, Ndi\params\ChannelRange,ParamDesc,,%RegionControl%
;HKR, Ndi\params\ChannelRange,default,,"0"
;HKR, Ndi\params\ChannelRange,type,,enum
;HKR, Ndi\params\ChannelRange\enum,"0",,%Default%
;HKR, Ndi\params\ChannelRange\enum,"010B",,%FCC/IC%
;HKR, Ndi\params\ChannelRange\enum,"010D",,%ETSI%
;HKR, Ndi\params\ChannelRange\enum,"0A0B",,%Spain%
;HKR, Ndi\params\ChannelRange\enum,"0A0D",,%France%
;HKR, Ndi\params\ChannelRange\enum,"0E0E",,%MKK%
;HKR, Ndi\params\ChannelRange\enum,"010E",,%MKK1%
;HKR, Ndi\params\ChannelRange\enum,"0309",,%Israel% 

HKR, Ndi\params\RegionCode, ParamDesc,,"%RegionCode%"
HKR, Ndi\params\RegionCode, default,,"-1"
HKR, Ndi\params\RegionCode, type,,enum
HKR, Ndi\params\RegionCode\enum,"0",,"%sku1%" 
HKR, Ndi\params\RegionCode\enum,"1",,"%sku2%" 
HKR, Ndi\params\RegionCode\enum,"2",,"%sku3%" 
HKR, Ndi\params\RegionCode\enum,"3",,"%sku4%" 
HKR, Ndi\params\RegionCode\enum,"4",,"%sku5%" 
HKR, Ndi\params\RegionCode\enum,"5",,"%sku6%"
HKR, Ndi\params\RegionCode\enum,"6",,"%sku7%"
HKR, Ndi\params\RegionCode\enum,"7",,"%sku8%"
HKR, Ndi\params\RegionCode\enum,"8",,"%sku9%"
HKR, Ndi\params\RegionCode\enum,"9",,"%sku10%"
HKR, Ndi\params\RegionCode\enum,"10",,"%sku11%"
HKR, Ndi\params\RegionCode\enum,"11",,"%sku12%"
HKR, Ndi\params\RegionCode\enum,"-1",,"%Default%"
 
;HKR, Ndi\params\AMSDUEnabled,ParamDesc,,"%AMSDUEnabled%"
;HKR, Ndi\params\AMSDUEnabled,default,,"2"
;HKR, Ndi\params\AMSDUEnabled,type,,enum 
;HKR, Ndi\params\AMSDUEnabled\enum,"0",,"%Disabled%"
;HKR, Ndi\params\AMSDUEnabled\enum,"1",,"%AMSDUEnabled_3839Bytes%" 
;HKR, Ndi\params\AMSDUEnabled\enum,"2",,"%AMSDUEnabled_Max%" 

HKR, Ndi\params\Aggregation,ParamDesc,,"%Aggregation%"
HKR, Ndi\params\Aggregation,default,,"2"
HKR, Ndi\params\Aggregation,type,,enum 
HKR, Ndi\params\Aggregation\enum,"0",,"%Disabled%"
HKR, Ndi\params\Aggregation\enum,"1",,"%AMSDUEnabled_4KBytes%" 
HKR, Ndi\params\Aggregation\enum,"2",,"%AMSDUEnabled_8KBytes%" 
HKR, Ndi\params\Aggregation\enum,"3",,"%AMPDUEnabled%" 

HKR, Ndi\params\RadioOffDisconnected,  ParamDesc, 0, "%RadioOffDisconnected%"
HKR, Ndi\params\RadioOffDisconnected,  default, 0, "0"
HKR, Ndi\params\RadioOffDisconnected,  min, 0, "0"
HKR, Ndi\params\RadioOffDisconnected,  max, 0, "86400"
HKR, Ndi\params\RadioOffDisconnected,  step, 0, "1"
HKR, Ndi\params\RadioOffDisconnected,  Base, 0, "10"
HKR, Ndi\params\RadioOffDisconnected,  type, 0, "dword"

;===========================================================================
; Strings section
;===========================================================================
[Strings]
MRVL = "Marvell"
Enabled = "Enabled"
Disabled = "Disabled"

;; Station Parameters
TxPowerLvlStr = "Tx Power Level"
TxAntennaStr = "Tx Antenna Select"
RxAntennaStr = "Rx Antenna Select" 
AdhocChannelStr = "Adhoc Creator Channel"
Channel = "Channel"
FragThsds = "Fragamentation Threshold"
DataRate = "Data Rate"
RTSThsds = "RTS Threshold"
AuthMode = "Authentication Mode"
;WirelessM = "Wireless Mode"
NetworkMode = "Operation Mode"
WepStatus = "WEP Status"
SSID = "SSID"
PreambleStr = "Preamble Select"
PowerMode = "Power Save Mode"
AdhocMode = "Ad-Hoc Mode"
AdhocMode_GMode = "Ad-Hoc G Mode"
AdhocMode_BMode = "Ad-Hoc B Mode only"
AdhocMode_NMode = "Ad-Hoc N Mode"
;AMSDUEnabled = "MSDU Aggregation"
;AMSDUEnabled_3839Bytes = "Enabled (3839 Bytes)" 
;AMSDUEnabled_Max = "Enabled (Device Max)" 
Aggregation = "Aggregation"
AMSDUEnabled_4KBytes = "AMSDU Enabled (4K)"
AMSDUEnabled_8KBytes = "AMSDU Enabled (8K)"
AMPDUEnabled = "AMPDU Enabled"
EWCTurboMode = "802.11n Turbo Mode"
;AMPDUSettings= "Packet Aggregation (A-MPDU)"
;Full = "Full"
;Partial = "Partial"
LowPower = "Low Power"
MediumPower = "Medium Power"
HighPower = "High Power"
VeryLowPower = "Very Low Power"
HTModeEnabled = "802.11n Network"
ChannelWidth = "Channel Width"
20MHz  = "20 MHz"
40MHz = "40 MHz"
Auto = "Auto"
ExtChannelOffset = "Extension Channel"
Below = "Lower"
Above = "Upper"
None = "None"
GuardInterval = "Guard Interval"
LongGI = "Standard"
ShortGI = "Short"
Antenna = "Antenna"
2by3 = "2by3"
Antenna_A = "Antenna A"
Antenna_B = "Antenna B"
2by2 = "2by2"
Aby2 = "A by 2"
Bby2 = "B by 2"
Open = "Open"
Shared = "Shared"
Adhoc = "Ad hoc"
Infrastructure = "Infrastructure"
ShortPreamble = "Short Preamble"
LongPreamble = "Long Preamble"
;Band11b = "11b"
;Band11g = "11g"
;Band11a = "11a"
Rate1 = "1 Mbps"
Rate2 = "2 Mbps"
Rate5 = "5.5 Mbps"
Rate11 = "11 Mbps"
Rate6 = "6 Mbps" 
Rate9 = "9 Mbps" 
Rate12 = "12 Mbps" 
Rate18 = "18 Mbps" 
Rate24 = "24 Mbps" 
Rate36 = "36 Mbps" 
Rate48 ="48 Mbps" 
Rate54 = "54 Mbps"
DriverDisk = "Marvell installation disk 1"
EncryptionType= "Encryption Type"
SwEncryption = "Sw Encryption"
HwEncryption = "Hw Encryption"
;RegionControl = "RegionControl"
IntlRoaming = "International Roaming"
Default = "Default"
RegionCode = "Region code"
sku1 = "SKU 1"
sku2 = "SKU 2"
sku3 = "SKU 3"
sku4 = "SKU 4"
sku5 = "SKU 5"
sku6 = "SKU 6"
sku7 = "SKU 7"
sku8 = "SKU 8"
sku9 = "SKU 9"
sku10 = "SKU 10"
sku11 = "SKU 11"
sku12 = "SKU 12"
;FCC/IC = "FCC/IC"
;ETSI = "ETSI"
;Spain = "Spain"
;France = "France"
;MKK = "MKK"
;MKK1 = "MKK1"
;Israel = "Israel" 
RadioOffDisconnected = "Radio Off if Disconnected"

;DefaultAdhocMediaModeStr = "Default Adhoc Media Mode"

MRVL8360USB.DeviceDesc       = "Marvell TOPDOG 802.11n WLAN Client Adaptors - USB"
BelkinN1USB.DeviceDesc       = "N1 Wireless USB Network Adapter"
LinksysNUSB.DeviceDesc       = "Wireless-N USB Network Adapter"
WN121TUSB.DeviceDesc         = "NETGEAR WN121T Wireless USB 2.0 Adapter"
WN111USB.DeviceDesc          = "RangeMax NEXT Wireless-N USB Adapter WN111"
N650USB.DeviceDesc           = "D-Link RangeBooster N USB Adapter"
AsusUSB1.DeviceDesc	= "ASUS 802.11n Network Adapter"
AsusUSB2.DeviceDesc	= "802.11n Network Adapter"
BuffaloUSB1.DeviceDesc	= "BUFFALO WLI-U2-G144N Wireless LAN Adapter"
BuffaloUSB2.DeviceDesc	= "BUFFALO WLI-U2-G300N Wireless LAN Adapter"
DLinkUSB.DeviceDesc	= "D-Link Wireless N USB Adapter DWA-130"

W8360USBx32.Service.DispName = "Marvell TOPDOG 802.11n WLAN Driver for Vista x86 (USB8x)"










 




