; NET8041.INF
;
; INF file for Windows XP
;
; SMC 10/100 PC Card
;
; Copyright 2001, SMC Networks,Inc.

[Version]
signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %V_SMC%
DriverVer   = 02/22/2001,1.00.0222.2001

[Manufacturer]
%V_SMC%=SMC

[SMC]
%*SMC8041.DeviceDesc%=SMC8041.ndi,PCMCIA\SMC-8041TX-10/100-PC-Card-3EF9

[SMC8041.ndi.NT]
Characteristics = 0x4
BusType         = 8
AddReg          = SMC8041.reg, common.reg
CopyFiles       = SMC8041.CopyFiles.Sys

[SMC8041.ndi.NT.Services]
AddService = SMC8041, 2, SMC8041.Service, SMC8041.EventLog
;,SMC8041.ndi.LogConfigOverride



[Common.reg]
HKR,Ndi\params\ConnectionType,ParamDesc,,"Connection Type"
HKR,Ndi\params\ConnectionType,default,,0
HKR,Ndi\params\ConnectionType,type,,enum
HKR,Ndi\params\ConnectionType\enum,0,,"AutoSense"
HKR,Ndi\params\ConnectionType\enum,8,,"100BaseTx"
HKR,Ndi\params\ConnectionType\enum,9,,"100BaseTx Full_Duplex"
HKR,Ndi\params\ConnectionType\enum,2,,"10BaseT (Twisted_Pair)"
HKR,Ndi\params\ConnectionType\enum,3,,"10BaseT Full_Duplex"


[SMC8041.ndi.LogConfigOverride]
LogConfig = SMC8041.LogConfigOverride

[SMC8041.LogConfigOverride]
IRQConfig=3,4,5,7,9,10,11,12,13,15
IOConfig=20@200-3FF%FFE0(3FF::)
ConfigPriority = NORMAL

;-------------------------------------------------------------------------------
; SMC8041 Drivers and Service
;
[SMC8041.reg]
HKR, Ndi,               Service,    0, "SMC8041"
HKR, Ndi\Interfaces,    DefUpper,   0, "ndis5"
HKR, Ndi\Interfaces,    DefLower,   0, "ethernet"
HKR, Ndi\Interfaces,    UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,    LowerRange, 0, "ethernet"
;HKR,               ,    CardType,   0, "1"
HKR,               ,    Pcmcia    , 0, "2"

[SMC8041.Service]
DisplayName     = %Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_AUTO_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\SMC8041.sys
LoadOrderGroup  = NDIS
AddReg          = TextModeFlags.reg

[SMC8041.CopyFiles.Sys]
SMC8041.sys

[DestinationDirs]
DefaultDestDir=11
SMC8041.CopyFiles.Sys = 12
;SMC8041.CopyFiles.Inf = 17

[SMC8041.EventLog]
AddReg = SMC8041.AddEventLog.reg

[SMC8041.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[TextModeFlags.reg]
HKR, , TextModeFlags, 0x00010001, 0x0001

[strings]
Service.DispName =   "SMC 10/100 PC Card Windows Driver"
; Provider
; Manufacturers
V_SMC="SMC"
; PNP Devices
*SMC8041.DeviceDesc="SMC 10/100 PC Card"