;; NETUSR79.INF
;;
;; U.S. Robotics 10/100 PCI NIC TX
;;
;; COPYRIGHT 2001 U.S. ROBOTICS CORPORATION

[version]
Signature   = "$CHICAGO$"
Compatible  = 1
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %USR%                                ;; for WHQL certified
CatalogFile = netusr79.cat                            ;; for WHQL certified
DriverVer   = 12/03/2001, 1.01.1203.2001

[Manufacturer]
%USR%    = USR

[ControlFlags]
ExcludeFromSelect     = PCI\VEN_1113&DEV_1216&SUBSYS_00ED16EC

[USR]
%USR7900.DeviceDesc%  = USR7900.ndi, PCI\VEN_1113&DEV_1216&SUBSYS_00ED16EC

;;****************************************************************************
;; Windows 9x
;;****************************************************************************
[USR7900.ndi]
DriverVer       = 12/03/2001, 1.01.1203.2001
AddReg          = USR7900.id.reg, USR7900.common.reg, USR7900.win.reg, USR7900.pci.reg
CopyFiles       = USR7900.CopyFiles9x

;;****************************************************************************
;; NT 5.0
;;****************************************************************************
[USR7900.ndi.NT]
DriverVer       = 12/03/2001, 1.01.1203.2001
AddReg          = USR7900.common.reg, USR7900.reg, USR7900.pci.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = USR7900.CopyFiles

[USR7900.ndi.NT.Services]
AddService      = USR7900, 2, USR7900.Service, USR7900.EventLog

[USR7900.CopyFiles9x]
USR7900.sys,,,2

[USR7900.CopyFiles]
USR7900.sys,,,2

;;----------------------------------------------------------------------------
;; USR7900 Parameters
;;----------------------------------------------------------------------------
;;****************************************************************************
;; Windows 9x parameters
;;****************************************************************************
[USR7900.id.reg]
HKR, Ndi,       DeviceID,       0,      "PCI\VEN_1113&DEV_1216&SUBSYS_00ED16EC"

[USR7900.pci.reg]
HKR, ,                                      AdapterType,    0, "5"
HKR,,TxPacketDesc,,"160"      ; 0xa0
HKR,,RxPacketDesc,,"120"      ; 0x78
HKR,,TxDmaDesc,,"320"         ; 0x140
HKR,,RxDmaDesc,,"40"          ; 0x28
HKR,,PacketsPerTxInt,,"10"    ; 0x0a
HKR,,PacketsPerRxInd,,"10"    ; 0x0a
HKR,,BurstLength,,"0"         ; 0 (Unlimited), 1 DW, 2 DW, 3 DW, ...

[USR7900.win.reg]
;; key,subkey,valuname,type,value
HKR, ,  AdapterCFID,     ,      12161113
HKR, ,  DriverDesc,     0,      "U.S. Robotics 10/100 PCI NIC TX"
HKR, ,  DevLoader,      0,      *ndis
HKR, ,  DeviceVxDs,     0,      USR7900.sys
HKR, ,  EnumPropPages,  0,      netdi.dll,      EnumPropPages

;;params
HKR, ,  MediaType,      0,      1
HKR, ,  AdapterType,    0,      5
HKR, ,  BusType,        0,      5

;; NDIS Info
HKR, NDIS,              MajorNdisVersion,       1,      03
HKR, NDIS,              MinorNdisVersion,       1,      0a
HKR, NDIS,              LogDriverName,          0,      "USR7900"

;; Interfaces
HKR, Ndi\Interfaces,    DefLower,               ,       "ethernet"
HKR, Ndi\Interfaces,    LowerRange,             ,       "ethernet"
HKR, Ndi\Interfaces,    DefUpper,               ,       "ndis3"
HKR, Ndi\Interfaces,    UpperRange,             ,       "ndis3"

;; Install sections
HKR, Ndi\Install,       ndis3,                 0,       "USR7900.ndis5"

;;****************************************************************************
;; USR7900 common parameters
;;****************************************************************************
[USR7900.common.reg]
HKR, Ndi\Params\MediaType,            ParamDesc, , "Media Type"
HKR, Ndi\Params\MediaType,            default,   , "0"
HKR, Ndi\Params\MediaType,            type,      , "enum"
HKR, Ndi\Params\MediaType\enum,       0,         , "AutoSense"
HKR, Ndi\Params\MediaType\enum,       1,         , "10BaseT"
HKR, Ndi\Params\MediaType\enum,       2,         , "10BaseT Full_Duplex"
HKR, Ndi\Params\MediaType\enum,       3,         , "100BaseTX"
HKR, Ndi\Params\MediaType\enum,       4,         , "100BaseTX Full_Duplex"
HKR, Ndi\Params\MediaType,            flag,     1, "20","00","00","00"

HKR, Ndi\Params\PowerManagement,      ParamDesc, , "PME Enable"
HKR, Ndi\Params\PowerManagement,      default,   , "1"
HKR, Ndi\Params\PowerManagement,      type,      , "enum"
HKR, Ndi\Params\PowerManagement\enum, 0,         , "Disabled"
HKR, Ndi\Params\PowerManagement\enum, 1,         , "Enabled"
HKR, Ndi\Params\PowerManagement,      flag,     1, "20","00","00","00"

HKR, Ndi\Params\WakeupFrame,          ParamDesc, , "Pattern Match Wakeup"
HKR, Ndi\Params\WakeupFrame,          default,   , "1"
HKR, Ndi\Params\WakeupFrame,          type,      , "enum"
HKR, Ndi\Params\WakeupFrame\enum,     0,         , "Disabled"
HKR, Ndi\Params\WakeupFrame\enum,     1,         , "Enabled"
HKR, Ndi\Params\WakeupFrame,          flag,     1, "20","00","00","00"

HKR, Ndi\Params\LinkOnChange,         ParamDesc, , "Link Wakeup(Off->On)"
HKR, Ndi\Params\LinkOnChange,         default,   , "1"
HKR, Ndi\Params\LinkOnChange,         type,      , "enum"
HKR, Ndi\Params\LinkOnChange\enum,    0,         , "Disabled"
HKR, Ndi\Params\LinkOnChange\enum,    1,         , "Enabled"
HKR, Ndi\Params\LinkOnChange,         flag,     1, "20","00","00","00"

HKR, Ndi\Params\LinkOffChange,        ParamDesc, , "Link Wakeup(On->Off)"
HKR, Ndi\Params\LinkOffChange,        default,   , "0"
HKR, Ndi\Params\LinkOffChange,        type,      , "enum"
HKR, Ndi\Params\LinkOffChange\enum,   0,         , "Disabled"
HKR, Ndi\Params\LinkOffChange\enum,   1,         , "Enabled"
HKR, Ndi\Params\LinkOffChange,        flag,     1, "20","00","00","00"

HKR, Ndi\Params\MagicPacket,          ParamDesc, , "Magic Packet Wakeup"
HKR, Ndi\Params\MagicPacket,          default,   , "1"
HKR, Ndi\Params\MagicPacket,          type,      , "enum"
HKR, Ndi\Params\MagicPacket\enum,     0,         , "Disabled"
HKR, Ndi\Params\MagicPacket\enum,     1,         , "Enabled"
HKR, Ndi\Params\MagicPacket,          flag,     1, "20","00","00","00"

HKR, Ndi\Params\FlowControl,          ParamDesc, , "Flow Control"
HKR, Ndi\Params\FlowControl,          default,   , "1"
HKR, Ndi\Params\FlowControl,          type,      , "enum"
HKR, Ndi\Params\FlowControl\enum,     0,         , "Disabled"
HKR, Ndi\Params\FlowControl\enum,     1,         , "Enabled"
HKR, Ndi\Params\FlowControl,          flag,     1, "20","00","00","00"

HKR, Ndi\Params\PriorityPacket,       ParamDesc, , "Priority Packet"
HKR, Ndi\Params\PriorityPacket,       default,   , "0"
HKR, Ndi\Params\PriorityPacket,       type,      , "enum"
HKR, Ndi\Params\PriorityPacket\enum,  0,         , "Disabled"
HKR, Ndi\Params\PriorityPacket\enum,  1,         , "Enabled"
HKR, Ndi\Params\PriorityPacket,       flag,     1, "20","00","00","00"

HKR,Ndi\params\VlanId,                ParamDesc,0, "VLAN ID"
HKR,Ndi\params\VlanId,                type,     0, "edit"
HKR,Ndi\params\VlanId,                default,  0, "0"
HKR,Ndi\params\VlanId,                LimitText,0, "4"
HKR,Ndi\params\VlanId,                UpperCase,0, "1"
HKR,Ndi\params\VlanId,                Optional, 0, "1"

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[USR7900.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "USR7900"

[USR7900.Service]
DisplayName     = %USR7900.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\USR7900.SYS
LoadOrderGroup  = NDIS


[USR7900.EventLog]
Addreg = USR7900.AddEventLog.reg

[USR7900.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000, %%SystemRoot%%\System32\netevent.dll
HKR,    ,   TypesSupported,     0x00010001, 7

;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
USR7900.CopyFiles9x          = 11
USR7900.CopyFiles            = 12
DefaultDestDir              = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
USR7900.sys=1
NETUSR79.INF=1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
USR                    = "U.S. ROBOTICS CORPORATION"

DISKNAME = "U.S. Robotics 10/100 PCI NIC TX Driver Diskette"

USR7900.DeviceDesc      = "U.S. Robotics 10/100 PCI NIC TX"
USR7900.Service.DispName = "U.S. Robotics 10/100 PCI NIC TX"
